®

CUSTOM FLASHING	®

FOR INTERNAL USE ONLY

CSR: 	 SO#: 	
Checked by:	

Customer: 	 City: 	
P.O. #: 	
Requested Ship Date: Ship Via:

ASC BUILDING PRODUCTS www.ascbp.com
Salem OR. Fax: 800.404.7443	Spokane WA. Fax: 800.767.1346

Indicate number of shears and bends

Line #: 	

MK:	(Use arrow	to indicate painted side)	(Show all degrees of inside angles)	
Price Per Piece: 			 Girth: 		 Number of Bends: 				 GA: 	
Color: 		 Qty: 	 Pitch: 			
Length: 		
Line #: 	

MK:	(Use arrow	to indicate painted side)	(Show all degrees of inside angles)	
Price Per Piece: 			 Girth: 		 Number of Bends: 				 GA: 	
Color: 		 Qty: 	 Pitch: 			
Length: 		
EXAMPLE

3⁄8” Hem	Painted Side
13⁄8”
90˚
61⁄8”	90˚
11⁄8”
* Open Hem (OH) shown in example	3⁄8” Hem

MK:	(Use arrow	to indicate painted side)	(Show all degrees of inside angles)	Price Per Piece: 	  Girth: 	9.375	
Number of Bends:   7	
GA: 	26 GA	
Color:  Winter White	
Qty: 	10	
Pitch: 			 Length: 	10’			

Shearing flat sheet (Shears) = 1
Break (Bends)= 1 per
Hem (Hooks) = 2 per
Show all dimensions
Show all degrees of inside angles
Specify roof pitch
Specify painted side
Specify open or closed hem for each hem
Salem & Spokane: 3⁄8” Hem
Sacramento & Tacoma: 1⁄2” Hem
* An Open Hem (OH) creates a “U” shape with a visible gap, while a Closed Hem (CH) folds the edge completely over, creating a flush, smooth edge.
AEP SPAN www.aepspan.com
Tacoma WA. Fax: 800.767.0791