STANDARD COLORS

ZINCALUME® Plus*
SRI: 64 • LRV: 67

CLASSIC BROWN
SRI: 29 • LRV: 7

WINTER WHITE
SRI: 88 • LRV: 74

MATTE BLACK
SRI: N/A • LRV: 5

LIGHT STONE
SRI: 70 • LRV: 53

CANYON RED
SRI: 45 • LRV: 16

DESERT BEIGE
SRI: 58 • LRV: 39

RUSTIC RED
SRI: 43 • LRV: 13

CHESTNUT BROWN
SRI: 36 • LRV: 12

OLD TOWN GRAY
SRI: 43 • LRV: 27

	 		

OLD ZINC GRAY
SRI: 43 • LRV: 22

WEATHERED COPPER
SRI: 32 • LRV: 11

SLATE GRAY
SRI: 32 • LRV: 13

TAHOE BLUE
SRI: 33 • LRV: 14

BLACKBERRY
SRI: 34 • LRV: 7

FINISHES DEVELOPED BY

EVERGLADE
SRI: 35 • LRV: 19

DENALI GREEN
SRI: 29 • LRV: 11

PREMIUM PRINTS1

FOREST GREEN
SRI: 36 • LRV: 8

COPPER PENNY1
SRI: 53 • LRV: 28

NATURAL RUST
SRI: 32 • LRV: 10

DRIFTWOOD
SRI: 53 • LRV: 36

RED CEDAR

SRI: 37 • LRV: 12

Premium prints subject to upcharge

Customer Service Center: 907-267-3000 | bpanchorage@ascprofiles.com

www.ascbp.com

1Please note these colors are batch sensitive (may have color variation) and are directional in nature. Different batches are not to be mixed on projects.
We recommend that you request a sample of current stocked material to review actual color before ordering to ensure color accuracy.

We are not responsible for color variations.

REPRESENTATION OF COLORS MAY VARY DUE TO PRINTING LIMITATIONS.
Sample color chips are available upon request.
Consult your ASC Building Products representative for more information.

SRI=Solar Reflective Index.  LRV=Light Reflectance Value.  GA= Gauge of Steel.  *Clear acrylic coated.
SRI values in accordance with ASTM E1980 and are based on independent testing. Cool Roof Rating Council (CRRC) performance values (for CA Title 24) are based on color families and will differ from those listed above. Please visit www.ascbp.com for additional information.

	

Skyline Roofing® panels feature the look of a standing seam panel with a concealed, through fastener design. With clean lines and lasting performance, Skyline Roofing panels have long been a top choice for residential roofing.

16" Net Coverage.
Roof Installation: Minimum 3:12 slope.
26ga available standard.
Subtle striations available.
Notching available.

Strata Rib® panel is a light gauge, exposed fastener panel with 36" coverage used in residential roof and wall applications.

36" Net Coverage.
Roof Installation: Minimum 3:12 slope.
Wall Installation: Horizontal or Vertical.
29ga available standard.
Matching polycarbonate panels available.

Nor-Clad® panel is a light gauge, exposed fastener panel with 36" coverage used in residential roof and wall applications.
36" Net Coverage.
Roof Installation: Minimum 3:12 slope.
Wall Installation: Horizontal or Vertical.
29ga available standard.
Matching polycarbonate panels available.

Klondike® Siding panel is an economical, structural, exposed fastened metal siding system suitable for extreme climates and is also ideal for residential and commercial, exterior or interior siding, wainscoting, and trailer skirting.

36" Net Coverage.
Wall Installation: Horizontal or Vertical.
29ga available standard.

TriLap® Steel Siding is a concealed fastener steel siding panel with the appearance of three wide- lapped boards. The product is for use in domestic and military residential construction and small, light commercial developments.

16" Net Coverage.
Wall Installation: Horizontal.
26ga available standard.

	ZINCALUME® PLUS	WINTER WHITE	LIGHT STONE	DESERT BEIGE	CHESTNUT BROWN	CLASSIC BROWN	MATTE BLACK	CANYON RED	RUSTIC RED	OLD TOWN GRAY	OLD ZINC GRAY	WEATHERED COPPER	SLATE GRAY	TAHOE BLUE	BLACKBERRY	EVERGLADE	DENALI GREEN	FOREST GREEN	COPPER PENNY	NATURAL RUST	DRIFTWOOD	RED CEDAR	
Limited Lifetime Warranty for residential applications.																							
16" SKYLINE ROOFING®	●				●	●	●		●		●	●	●	●			●	●	●	●		●	
36" STRATA RIB®	●	●	●	●	●	●	●	●	●	●	●	●	●	●	●	●	●	●	●	●	●	●	
36" NOR-CLAD®	●	●	●	●	●	●	●	●	●	●	●	●	●	●	●	●	●	●	●	●	●	●	
36" KLONDIKE® SIDING	●	●	●	●	●	●	●	●	●	●	●	●	●	●	●	●	●	●	●	●	●	●	
16" TRILAP® STEEL SIDING	●				●	●	●		●		●	●	●	●			●	●	●	●		●	

All information stated in the color card is correct at time of printing and subject to change without notice.
©2024 ASC Profiles LLC All rights reserved. Spectrascape® is a registered trademark of Steelscape, LLC. ZINCALUME® is a registered trademark of BlueScope Steel Ltd. 0824 web (CC160)

www.ascbp.com