CUSTOM FLASHING

FOR INTERNAL USE ONLY

CSR:	 SO#:   	
Checked by:  	

Customer:	 City:  	

Line #:  	

MK:	(Use arrow ➞ to indicate painted side)	(Show all degrees of inside angles)	
Price Per Piece:  	                                Girth:	 Number of Bends:  	                                  GA:   	 
Color:		 Qty:		 Pitch:  		
Length:  		

Line #:  	

MK:	(Use arrow ➞ to indicate painted side)	(Show all degrees of inside angles)	
Price Per Piece:  	                                Girth:	 Number of Bends:  	                                  GA:   	 
Color:		 Qty:		 Pitch:  		
Length:  		

P.O. #:    	 Requested Ship Date:   	 Ship Via:  	

EXAMPLE

3⁄8″ Hem
Painted Side
13⁄8″
90˚
61⁄8″	90˚
11⁄8″
3⁄8″ Hem

MK:	(Use arrow ➞ to indicate painted side)	(Show all degrees of inside angles)	Price Per Piece:  		                                 Girth:	9.375
Number of Bends:	7
GA: 	26 GA
Color:     Winter White
Qty: 	10	
Pitch:		 Length: 	10’		

ASC BUILDING PRODUCTS www.ascbp.com

Indicate number of shears and bends
Shearing flat sheet (Shears) = 1
Break (Bends)= 1 per

Hem (Hooks) = 2 per
Show all dimensions
Show all degree of bend
Specify roof pitch
Specify painted side
Specify open or closed hem for each hem
Anchorage, Salem, Spokane: 3⁄8″ Hem
Salt Lake City: 7⁄16″ Hem
Sacramento, Tacoma, Fontana: 1⁄2″ Hem
AEP SPAN www.aepspan.com

Salem OR. Fax: 800.404.7443	Spokane WA. Fax: 800.767.1346	Anchorage AK. Fax: 907-267-3011	Tacoma WA. Fax: 800.767.0791