®

TRILAP® STEEL SIDING

TriLap® Steel Siding
TriLap® Steel Siding is a concealed fastener steel siding panel with the appearance of three wide-
lapped boards. This long-lasting and durable panel
is recommended for residential and light commercial developments.

FEATURES AND BENEFITS
16" coverage siding panel.
Siding Installation: Horizontal
26ga available as standard in our Dura Tech xl colors and ZINCALUME® Plus.
Red Cedar Woodgrain print is available as a standard color option in 26ga.
Standard flashing colors available.
16" coverage means fewer panels and less labor to install.
Limited Lifetime Warranty for residential applications.
Custom manufactured panel lengths: 6'-0" to 46'-0".

16" Panel Coverage

Customer Service Centers I Anchorage, AK: 907-267-3000
Salem, OR: 503-390-7174 or 800-272-7023 I Spokane, WA: 509-536-4097 or 800-776-8771

www.ascbp.com

Keeps the Heat Out and the Color Brilliant.
Superior color retention and resistance to chalk and fade.
Energy saving cool colors reduce the demand for energy.
Standard Colors

ZINCALUME® Plus
26 Gauge

Rustic Red
26 Gauge

Old Zinc Gray
26 Gauge

Weathered Copper
26 Gauge

Classic Brown
26 Gauge

Chestnut Brown
26 Gauge

Slate Gray
26 Gauge

Tahoe Blue
26 Gauge

Denali Green
26 Gauge

Forest Green
26 Gauge

Premium Colors (Subject to upcharge)

Matte Black
26 Gauge

Copper Penny*
26 Gauge

Natural Rust*
26 Gauge

TRILAP® STEEL SIDING IS ENGINEERED TO OUTPERFORM WOOD, ALUMINUM OR VINYL IN THE RUGGED ALASKAN CLIMATE.

Red Cedar* (Woodgrain Print) 26 Gauge

REPRESENTATION OF COLORS MAY VARY DUE TO PRINTING LIMITATIONS.
Sample color chips are available upon request. Consult your ASC Building Products representative for more information.

* Please note these colors are batch sensitive (may have color variation) and are directional in nature. Different batches are not to be mixed on projects. We recommend that you request a sample of current stocked material to review actual color before ordering to ensure color accuracy. We are not responsible for color variations.

Solar Reflective Index (SRI) values in accordance with ASTM E1980 and are based on independent testing. Cool Roof Rating Council (CRRC) performance Light Reflectance Value (LRV) values (for CA Title 24) are based on color families and will differ from those listed online.

Installation Guide with Flashings and

www.ascbp.com

Details available at

ASC Building Products is Proudly Distributed by:

©2024 ASC Profiles LLC. All rights reserved. ZINCALUME® is a registeredtrademark of BlueScope Steel Ltd. 0224 web (PS136)

www.ascbp.com

TRILAP® STEEL SIDING

®