R42 Vented Ridge	SF41 Support Flashing	TR41 Transition (High-Low)	

9"
1-1/2"  3"

Pitch Required	1"

1-3/4"

5-1/4"	

7"	16-1/2"

Pitch Required	

FLASHING LOCATIONS
ASC Building Products recommends all properly installed roofs include flashings. Visit	®

www.ascbp.com for a full list of trims, flashings, installation guides and product details.

TR43 Transition (Low-High)	V41 Valley	ZL41 “Z” Clip	

16-1/2"
7"

Pitch Required	
1/2"
1"	19-1/2"

Pitch Required	2 1/8"
1-3/4"

2” Length	2 1/8"	

HIP/RIDGE

ENDWALL

VALLEY FLASHING

TOP CLOSURE

PIPE FLASHING

GABLE TRIM

METAL ROOFING AND SIDING PRODUCTS

			
EAVE FLASHING

Z41 “Z” Closure	B1 Base Trim	C13 C-Metal	

2-1/8"

1-3/4"

2-1/8"	

2-1/8"

1"	1/2"	
3-1/2"
1" 
1"	

G19 Gable	IC2 Inside Corner	OC2 Outside Corner	
3-1/2" 1/2"
4-3/4"

3/4"	

3-1/2"	

3-1/2"	

C-METAL

DOUBLE TRACK COVER

SINGLE TRACK COVER

OIL CANNING: All flat metal surfaces can display waviness commonly referred to as “oil canning.” Oil canning is an inherent characteristic of steel products, not a defect, and therefore is not a cause for panel rejection.

SW8 Sidewall	E6 Eave	EW6 Endwall	

5-1/4"
5"	
5-3/4"

4"
Pitch Required	3/4"	

4-1/2"

6"

Pitch Required	

BOTTOM CLOSURE

SIDEWALL

BASE TRIM

Pitch Required = Trim manufactured based on roof pitch. Please ensure roof pitch provided at time of order entry.

R8 Ridge	V6 W-Valley	B6 Drip Edge	

10"

Pitch Required	

3/4"
20-3/4"

Pitch Required	

4-1/8"

1-5/8"
3/4"	

INSTALLATION GUIDES & RESOURCES

C6 C-Metal	G8 Gable	G9 Sculptured Gable	

3-7/8"
1-3/8"

1-1/4"	4-7/8"	7/8"
1-3/4"
5-1/4"

3/4"	1"	6"	3-1/2"
2-1/8"

1-1/2"	3-1/2"

2-1/8"	

This tri-fold is meant to display the most common trims and flashings but is not all inclusive. Scan the QR code to access all of our installation guides and resources, which contain a full list of metal roof flashing, trims & accessories.

INSIDE CORNER

®

OUTSIDE CORNER

JAMB TRIM

IC7 Inside Corner	OC7 Outside Corner	SW7 Sidewall	

4-1/4"
1-3/4"
3/4"	

4-3/16"

1-15/16"
5/8"	

5-5/8"
5"
2-1/8" 1"	

Customer Service Centers
Salem, OR 503-390-7174 or 800-272-7023 • bpsalem@ascprofiles.com

Spokane, WA 509-536-4097 or 800-776-8771 • bpspokane@ascprofiles.com

All information stated in the brochure is correct at time of printing and subject to change without notice.
©2025 ASC Profiles LLC All rights reserved. Spectrascape® is a registered trademark of Steelscape, LLC. ZINCALUME® is a registered trademark of BlueScope Steel Ltd. 0225 web (BR315)

Color Key												36" - Nu-Wave® Corrugated	
Dura Tech™ xl (SMP)	12" - Skyline Roofing®	16" - Skyline Roofing®	
24" - 21⁄2" Corrugated										
ColorGuard 25
with Spectrascape® (Polyester)				24" - Delta Rib™	
36" - Nor-Clad®		
36" - Strata Rib®		
36" - Delta Rib™ III		36" - PBR Panel		
Dura Tech™ nt (SMP)													
ZINCALUME® Plus (Unpainted product)													
Premium Color (Subject to upcharge)													
Colors & Gauges	26	26	29	26	29 	26  		29			26  		29			26 	 29 	26 	26 	 26 	
ZINCALUME® Plus			AK/CA OR/WA		1	WA		AK/CA OR/WA			AK/CA OR/WA					
Winter White	
		CA OR/WA				
AK/CA OR/WA	OR WA	AK/CA OR/WA	WA					
Surf White	
						OR WA			OR WA						
Light Stone	
		CA OR/WA				AK	CA OR/WA	AK	CA OR/WA					
Desert Beige	
						AK/CA OR/WA	OR WA	AK/CA OR/WA	WA					
Cascade Gray							OR			OR						
Taupe							CA OR/WA		CA OR/WA						
Patina Steel	
		CA OR/WA				CA OR/WA		CA OR/WA						
Chestnut Brown	
		AK/CA OR/WA				AK/CA OR/WA	OR WA	AK/CA OR/WA	WA					
Classic Brown	
		AK/CA OR/WA				AK/CA OR/WA		AK/CA OR/WA						
Matte Black*			AK/CA OR/WA				AK/CA OR/WA		AK/CA OR/WA						
Canyon Red	
						AK/CA OR/WA		AK/CA OR/WA						
Rustic Red	
		AK/CA OR/WA				AK/CA OR/WA	OR WA	AK/CA OR/WA	WA					
Old Town Gray	
		CA OR/WA				AK/CA OR/WA	OR WA	AK/CA OR/WA	WA					
Old Zinc Gray	
		AK/CA OR/WA				AK/CA OR/WA		AK/CA OR/WA							
Weathered
Copper	
		AK/CA OR/WA				AK/CA OR/WA		AK/CA OR/WA		
					
Slate Gray	
		AK/CA OR/WA			CA	AK/CA OR/WA		AK/CA OR/WA							
Tahoe Blue	
		AK/CA OR/WA			WA	AK/CA OR/WA		AK/CA OR/WA		OR					
Everglade	
		CA OR/WA				AK/CA OR/WA		AK/CA OR/WA							
Denali Green	
		AK/CA OR/WA				AK/CA OR/WA	OR WA	AK/CA OR/WA	WA						
Forest Green	
		AK/CA OR/WA		
		AK/CA OR/WA	OR WA	AK/CA OR/WA	WA						
Copper Penny**	
		AK/CA OR/WA				AK/ OR/WA		AK/ OR/WA						
Natural Rust**			AK/CA OR/WA	1				AK WA			AK WA					
	
IronOx2													2	
	Production Locations					Sacramento, CA, Spokane, WA					Sacramento, CA, Salem, OR					

AK - Anchorage, Alaska
CA - Sacramento, California OR - Salem, Oregon
WA - Spokane, Washington

Also available in 32" net coverage.
IronOx is black steel (uncoated and unpainted),	Salem, OR	Multiple Locations (See Key)	Sacramento, CA		Sacramento, CA	Multiple Locations (See key)	Salem, OR	Multiple Locations (See key)		
Salem, OR		Sacramento, CA	Sacramento, CA	

that rusts naturally. No warranty is offered or implied. Only available in 22 gauge Nu-Wave® Corrugated.
* Matte Black is not a rated product by the Cool Roof Rating Council.
** Please note these colors are batch sensitive (may have color variation) and are directional in nature. Different batches are not to be mixed on projects.

www.ascbp.com

REPRESENTATION OF COLORS MAY VARY DUE TO PRINTING LIMITATIONS.
Sample metal color chips are available upon request.
Consult your ASC Building Products representative for more information.

We recommend you request a sample of current stocked material to review actual color before ordering to ensure color accuracy. We are not responsible for color variations.

Strata Rib®

9"

3/4"

36" Coverage

Nor-Clad®

PRODUCTS

COLOR KEY

B1 Base Trim	C1 7/8” C-Metal	E1 Eave	E2 Eave	E3 Eave	E4 Eave	E5 Eave	

2-1/8"
1"	1/2"	2"

7/8"

1"	1-1/2"

3"

1/2"
Pitch Required	2"

4-3/8"

Pitch Required	1/2"	1-3/8"

1-3/8"
Pitch Required	1/2"	2"

2"
1/2"
Pitch Required	3"

3"
Pitch Required	1/2"	

COMMON TRIMS AND FLASHINGS

9"

5/8"

36" Coverage

ER1 Residential 3” Eave	ER2 Residential 4” Eave	EW1 Endwall	EW2 Residential Endwall	EW17 Vented Endwall	G1 Gable	G3 Gable	G4 Residential Gable	G18 Chalet Gable	IC1 Inside Corner	
2"

3-3/8"
1/2"
Pitch Required	3"

4-3/8"

Pitch Required	1/2"	
4"
1-1/8"
1/2"	2"
Pitch Required 1/2"	3/4"	

4"

5"
Pitch Required	
4"
6-3/4"

1-1/8"  1-7/8"	4" 1-1/8" 5/8"

5"

5/8"	4"
1-1/4"	1/2"
2-3/4"

1/2"	2"	5/8"
1-1/8"

4"

1/2"	3/4"
1-5/8"	6"
3-7/8"
5/8"	

4"
1-1/8"
5/8"	

See product installation guides for full list of options at www.ascbp.com.

Delta Rib™

9"

Delta Rib™ III

36" Coverage

3/4"

8"

13/16"

24" Coverage

IC2 Inside Corner	OC1 Outside Corner	OC2 Outside Corner	PB3 Pitch Break (High-Low)	PB4 Pitch Break (Low-High)	PF2 Peak Flashing	PF3 Vented Peak	R1 Ridge	R2 Vented Ridge	

3-1/2"	

4"

1-1/8"
5/8"	

3-1/2"	

5"

6"

Pitch Required	
6"
5"

Pitch Required	Varies

Varies

1/2"	Pitch Required	
Varies
Varies
1-1/8" 1-7/8"
1/2"
Pitch Required	
2"	2-1/8"
1/2"	1-7/8"
1/2"
13/16"
Pitch Required	
6-3/4"
1-7/8"
1-1/8"

Pitch Required	

21⁄2" Corrugated

2-2/3"

1/2"

21-1/3" Roof Coverage 24" Wall Coverage

Nu-Wave® Corrugated

2-11/16"

7/8"

32" Roof Coverage
34-1/3" Wall Coverage

R3 Standard Ridge	R4 Residential Ridge	SW1 Sidewall	SW2 Residential Sidewall	TC1 Single Track Cover	TC2 Single Track Cover	TC3 Double Track Cover	V1 W-Valley	V2 Residential Valley	

7"

Pitch Required	
3-3/4"

1/2"
3-1/2"

Pitch Required	

4"
1/2"	1/2"
1-1/8"	2"	3/4"	

4"
3"
1-1/8" 5/8"	1-1/2"  3-13/16"
1-7/16"

3-13/16"	1-1/2"
2-1/4"	1-7/16"

3-13/16"	1-1/2"

7-3/16"
2-1/2"
2-3/8"	

1"
13"

Pitch Required	

1"	19-7/16"

Pitch Required	

B16 Base Trim	C16 C Trim	E16 Narrow Eave	E17 Wide Eave	E18 Snow Eave	E19 Nosed Eave	E21 Nosed Eave	E22 Nosed Eave	EW16 Endwall	

3"
1-1/8"
1/2"	
3"
1-1/8"

1"	
2"

1-1/8"
1/2"
Pitch Required	4"

3"
5/8"
Pitch Required	5-1/8"

1-1/4"
1-3/4"
Pitch Required	1/2"	3-1/2"

1-1/4"
Varies
5/8"
Pitch Required	3-3/4"

1-1/4"
1-1/2"
5/8"
Pitch Required	
3-3/4"

1" 1-1/4"
5/8"
Pitch Required	

4"

5-1/2"
Pitch Required	

Wider panel available. 29-1/3" roof coverage and 32" wall coverage. See matrix for color options.

EW17 Vented Endwall	G5 Adjustable Gable	G16 Narrow Gable	G17 Standard Gable	G18 Chalet Gable	PF16 Peak Flashing	PF18 Vented Peak	R16 Hip/Ridge	R17 Vented Ridge	

4"
6-3/4"
1-1/8"	1-7/8"
Pitch Required	6"

4"

1/2"	1/2"
1"	1"

3"

1/2"	2-1/4"
1-1/8"	3/4"
4"	3/8"

1/2"	3/4"	1-5/8"
3-7/8"	6"
5/8"	Varies

Varies

1/2"
Pitch Required	
Varies
Varies
1-1/8"  2"

1/2"	Pitch Required	

5-1/2"

Pitch Required	
6-3/4"
2"
1-1/8"

Pitch Required	

Skyline Roofing®

12"

1-1/4"

36" Coverage

R18 Narrow Ridge	SS1 Starter Strip	SW16 Sidewall	SW17 Sidewall	SW18 Sidewall	TR16 Transition (High-Low)	TR17 Transition (Low-High)	V16 Valley	Z17 Solid Zee Closure	Z18 Perforated Zee	

4-7/16"

7/8"

Pitch Required	

1"

2-1/2"	

4"
2-1/4"
1-1/8"	3/4"	

4"
2-1/4"
2-1/8"  3/4"	

4"
2-1/4"

2-1/2"
1"	
5"
Varies

Pitch Required	

Varies	5"

Pitch Required	

1"
12"

Pitch Required	
1-3/16"	2-13/16"

Colors may vary
1"	1-3/16"		Varies 1"	Colors may vary
Pitch Required	

1"

12" or 16" Coverage

PBR Panel

Design Span® hp

Available as ribbed or striated panel. Ribbed shown here.

1-3/4"

12", 16", 17", or 18" Coverage
Available as flat or striated panel. Striated shown here.

AL41 Angle Cleat	B41 Drip Flashing	CF41 Counter Flashing	G41 Gable	L41 Closure	OL41 Offset Cleat	R41 Ridge	
24ga - 22ga PVDF colors available for PBR Panel, Skyline Roofing hp and Design Span hp. See ascbp.com for color chart.

1-1/2"

1-1/4"

1-1/2"

2-3/8"

5-1/2"

3-1/2"

5/8"

2"

6"

2"

1"
1"

1/2"
5-7/8"

3/4"

8-1/2"

1-3/4"

2-1/4"

5/16"

13/16"

Pitch Required

Striated: Striations are the small ridges on panels engineered to help minimize the appearance of oil canning.