V41 Valley	G41 Gable	SF41 Support Flashing	

1/2″
1″
19-1/2″

Pitch Required	1-1/2″
1-1/4″
1/2″
5-7/8″

3/4″	1″

1-3/4″

5-1/4″	

FLASHING LOCATIONS
ASC Building Products recommends all properly installed roofs include flashings.	®
Visit www.ascbp.com for installation guides and product details.

VALLEY FLASHING

TOP CLOSURE

PIPE FLASHING

GABLE TRIM

UNIVERSAL

 METAL ROOFING AND SIDING PRODUCTS

5-1/2″	

2″	
6″		

CF41 Counter Flashing	B41 Drip Flashing	TR41 Transition (High-Low)	

3-1/2″

1″
1″	

2″	

7″
16-1/2″

Pitch Required	

EAVE FLASHING

TR43 Transition (Low-High)	C13 C-Metal	G19 Gable	

16-1/2″

Pitch Required	

7″			
3-1/2″		
3-1/2″	
1/2″	
		1″			4-3/4″			
			1″		
3/4″			

IC11 Universal Inside Corner	OC11 Universal Outside Corner	SW8 Sidewall	

6-3/4″	

6-3/4″	

5-1/4″

5″	

UNIVERSAL HIP/RIDGE

BOTTOM CLOSURE

ENDWALL

UNIVERSAL SIDEWALL

C-METAL

DOUBLE TRACK COVER

Color Key															36" Nu-Wave® Corrugated	
Dura Tech™ xl (SMP)	12" Skyline Roofing®	16" Skyline Roofing®														
ColorGuard 25
with Spectrascape® (Polyester)			21⁄2" Corrugated	24" Delta Rib™		®			36" Strata Rib®			36" Delta Rib™ III		36" PBR Panel		
Dura Tech™ nt (SMP)						36" Nor-Clad										
ZINCALUME® Plus (Unpainted product)																
Premium Color (Subject to upcharge)																
Colors & Gauges	26	26	29	26	29	26	29	26	29	26	29	26	26	26	
ZINCALUME®
Plus	
		 AK/CA 		
1	
WA		AK/CA OR/WA		AK/CA OR/WA						
			OR/WA													
Winter White			CA					AK/CA OR/WA	OR		AK/CA	WA							
			OR/WA						WA		OR/WA								
Surf White								OR WA			OR								
											WA								
Light Stone			CA OR/WA					AK	CA		AK	CA							
									OR/WA			OR/WA							
Desert Beige								AK/CA OR/WA	OR		AK/CA	WA							
									WA		OR/WA								
Cascade Gray								OR			OR								
Taupe								CA OR/WA			CA								
											OR/WA								
Patina Steel			CA OR/WA					CA OR/WA			CA								
											OR/WA								
Chestnut Brown			AK/CA OR/WA					AK/CA OR/WA	OR		AK/CA	WA							
									WA		OR/WA								
Classic Brown			AK/CA OR/WA					AK/CA OR/WA			AK/CA								
											OR/WA								
Matte Black			AK/CA OR/WA					AK/CA OR/WA			AK/CA								
											OR/WA								
Canyon Red								AK/CA OR/WA			AK/CA								
											OR/WA								
Rustic Red			AK/CA					AK/CA OR/WA	OR		AK/CA	WA							
			OR/WA						WA		OR/WA								
Old Town Gray			CA					AK/CA OR/WA	OR		AK/CA	WA							
			OR/WA						WA		OR/WA								
Old Zinc Gray			AK/CA					AK/CA OR/WA			AK/CA								
			OR/WA								OR/WA								
Weathered
Copper			AK/CA					AK/CA OR/WA			AK/CA								
			OR/WA								OR/WA								
Slate Gray			AK/CA			CA		AK/CA OR/WA			AK/CA								
			OR/WA								OR/WA								
Tahoe Blue			AK/CA			WA		AK/CA OR/WA			AK/CA		OR						
			OR/WA								OR/WA								
Everglade			CA					AK/CA OR/WA			AK/CA								
			OR/WA								OR/WA								
Denali Green			AK/CA					AK/CA OR/WA	OR		AK/CA	WA							
			OR/WA						WA		OR/WA								
Forest Green			AK/CA					AK/CA OR/WA	OR		AK/CA	WA							
			OR/WA						WA		OR/WA								
Copper Penny*			AK/CA					AK/CA OR/WA			AK/CA								
			OR/WA								OR/WA								
Natural Rust*			AK/CA OR/WA	1				AK WA		AK WA							
IronOx2														2	

SINGLE TRACK COVER

BASE TRIM

OIL CANNING: All flat metal surfaces can display waviness commonly referred to as “oil canning.” “Oil canning” is an inherent characteristic of steel products, not a defect, and therefore is not a cause for panel rejection.

EW6 Universal Endwall	V6 W-Valley	R8 Ridge	

4-1/2″

6″
Pitch Required	

3/4″
20-3/4″
Not available for PBR Panel
Pitch Required	

10″

Pitch Required	

JAMB TRIM

E6 Eave	B6 Drip Edge	SB1 Snow Break	
5-3/4″

4″
Pitch Required	3/4″	

4-1/8″

1-5/8″
3/4″	2″	3-1/2″
1-1/2″

Works with most panels and offered as a convenience. ASC Building Products doesn’t provide any installation guidance or engineering for them.	

INSIDE CORNER

ASC Building Products is Proudly Distributed by:

OUTSIDE CORNER

 	 	

SW7 Sidewall	G8 Gable	OC7 Outside Corner	

5-5/8″

5″
2-1/8″  1″	4-7/8″	7/8″
1-3/4″
1/2″
5-1/4″

3/4″	

4-3/16″

1-15/16″
5/8″	

®

IC7 Inside Corner	C6	C-Metal	G9 Sculptured Gable	
						6″			
			3-7/8″	1″	2-1/8″			3-1/2″	
4-1/4″	1-3/8″			5/8″					
1-3/4″
3/4″		
1-1/4″					1-1/2″
2-1/8″	3-1/2″	

Customer Service Centers

Anchorage, Alaska (AK) Sacramento, California (CA) Salem, Oregon (OR) Spokane, Washington (WA)

Production Locations

Salem, OR
Multiple Locations (See Key)

Sacramento, CA

Sacramento, CA, Spokane, WA Sacramento, CA

Multiple Locations (See key)

Salem, OR

Multiple Locations (See key)

Sacramento, CA, Salem, OR

Salem, OR

Sacramento, CA
Sacramento, CA

Footnotes:

Salem, OR 503-390-7174 or 800-272-7023 • bpsalem@ascprofiles.com
Spokane, WA 509-536-4097 or 800-776-8771 • bpspokane@ascprofiles.com

All information stated in the brochure is correct at time of printing and subject to change without notice.
©2023 ASC Profiles LLC All rights reserved. Spectrascape® is a registered trademark of Steelscape, LLC. ZINCALUME® is a registered trademark of BlueScope Steel Ltd. 0823 Web (BR315)

Also available in 32" Net Coverage.
IronOx is black steel (uncoated and unpainted), that rusts naturally. No warranty is offered or implied. Only available in 22 GA Nu-Wave® Corrugated.

Dura Tech™ 5000/mx (PVDF) 24ga & 22ga colors available for:
Skyline Roofing hp, Nu-Wave Corrugated, PBR Panel, and Design Span hp.

www.ascbp.com

REPRESENTATION OF COLORS MAY VARY DUE TO PRINTING LIMITATIONS. Sample metal color chips
are available upon request. Consult your ASC Building Products representative for more information.

See ascbp.com for Dura Tech™ 5000/mx color chart.

* Please note, these colors are batch sensitive (may have color variation) and are directional in nature. Different batches are not to be mixed on projects. We recommend you request a sample of current stocked material to review actual color before ordering to ensure color accuracy.
WE ARE NOT RESPONSIBLE FOR COLOR VARIATIONS.

Strata Rib®

TRIM & FLASHING COLOR KEY:

Wider panel only available in

Nor-Clad®

TRIM & FLASHING COLOR KEY:

Delta Rib™ III

TRIM & FLASHING COLOR KEY:

Delta Rib™

TRIM & FLASHING COLOR KEY:

21⁄2" Corrugated

TRIM & FLASHING COLOR KEY:

26ga ZINCALUME® Plus and 29ga Natural Rust

9″
36″ Net Coverage

13/16″
8″

24″ Net Coverage

2-2/3″
21-1/3″ Roof Coverage 24″ Wall Coverage

1/2″

R16 Hip/Ridge	R18 Narrow Ridge	R17 Vented Ridge	Z16 Perforated Zee	Z17 Solid Zee Closure	G16 Narrow Gable	G17 Standard Gable	

5-1/2″

Pitch Required	

4-7/16″

7/8″

Pitch Required	

6-3/4″
1-1/8″ 2″

Pitch Required	
Varies

1-3/16″
Colors may vary

1″	Pitch Required	
2-13/16″
1-3/16″
Colors may vary
1″	1/2″
1″	1″

3″

1/2″	2-1/4″
1-1/8″  3/4″
4″	3/8″

1/2″	

29-1/3″ Roof Coverage 32″ Wall Coverage

3/4″

9″
36″ Net Coverage

R1 Universal	Ridge	R3 Standard	Ridge	R4 Residential	Ridge	R2 Vented	Ridge	C1 7/8”	C-Metal	V1	W-Valley	V2 Reside	ntial	Valley	

Pitch Required	

7″				

1-1/8″

Pitch Required	

6-3/4″	

1-7/8″			2″	

Pitch Required	

1″	

13″	

Pitch Required	

1″	

19-7/16″	
	2″	2-1/8″				3-3/4″														
1/2″
1/2″		1-7/8″			1/2″		
3-1/2″				7/8″									

Pitch Required		13/16″			
Pitch Required							1″								

B1 Base Trim	E1 Eave	E2 Eave	E3 Eave	E4 Eave	E5 Eave	ER1 Residential 3” Eave	ER2 Residential 4” Eave	

2-1/8″

1″	1/2″	1-1/2″

3″

Pitch Required	1/2″	2″

4-3/8″

Pitch Required	1/2″	1-3/8″

1-3/8″

1/2″
Pitch Required	2″

2″

1/2″
Pitch Required	3″

3″

Pitch Required	1/2″	2″

3-3/8″

1/2″
Pitch Required	3″

4-3/8″

1/2″
Pitch Required	

5/8″

9″

36″ Net Coverage

3/4″

G1 Gable	G3 Gable	G4	Residential	Gable	PF2	Peak	Flashing	OC1 4” x 4” Outside Corner	OC2 Universal Outside Corner	IC1 4” x 4” Inside Corner	

5″		4″	
1-1/8″	5/8″	

2-3/4″	4″	
1-1/4″	
1/2″	

4″

1/2″	2″
1-1/8″	5/8″
3/8″	

Varies	
Varies 3/8″

Pitch Required	

4″	

3-1/2″	

4″	
														1-1/8″		1-1/8″	
5/8″	3/8″				1/2″							1/2″		5/8″		5/8″	

2-2/3″

IC2 Universal Inside Corner	SW1 Universal Sidewall	SW2 Residential Sidewall	EW1 Universal Endwall	EW2 Residential Endwall	PB3 Pitch Break (High-Low)	PB4 Pitch Break (Low-High)	

3-1/2″	

4″

1/2″	1/2″
1-1/8″	2″	3/4″	

4″

3″
1-1/8″  5/8″	
4″
1-1/8″
1/2″	2″
1/2″  3/4″
Pitch Required	

4″

5″
Pitch Required	

5″

6″

Pitch Required	
6″
5″

Pitch Required	

1/2″

Nu-Wave® Corrugated	TRIM & FLASHING COLOR KEY:

2-11/16″

32″ Roof Coverage 34-1/3″ Wall Coverage

7/8″

G18 Chalet Gable	V16 Valley	E16 Narrow Eave	E17 Wide Eave	E18 Snow Eave	E19 Notched Eave	TR16 Transition (High-Low)	
3/4″
1-5/8″
3-7/8″	6″
5/8″	

1″
12″

Pitch Required	
2″

1-1/8″
1/2″
Pitch Required	4″

3″

5/8″
Pitch Required	5-1/8″

1-1/4″
1-3/4″
Pitch Required	1/2″	3-1/4″

1-1/4″ No customs Varies available
Pitch Required	5/8″	

5″
Varies

Pitch Required	

24ga and 22ga in Dura Tech™ 5000/mx. (Colors not shown — see ascbp.com for color chart)

PBR Panel

TRIM & FLASHING COLOR KEY:

Additional lead times and freight charges apply

12"

1-1/4″

36" Net Coverage

Skyline Roofing®

TRIM & FLASHING COLOR KEY:

Design Span® hp

TRIM & FLASHING COLOR KEY:

1-3/4"

24ga and 22ga in Dura Tech™ 5000/mx. (Colors not shown — see ascbp.com for color chart)
Additional lead times and freight charges apply

1"

TR17 Transition (Low-High)	SW16 Sidewall	SW17 Sidewall	SW18 Sidewall	EW16 Endwall	EW17 Vented	Endwall	B16	Base	Trim	PF16	Peak Flashing	

4″

6-3/4″
1-1/8″
Pitch Required						Varies	

Varies

Pitch Required	
5″	
4″	

2-1/4″
1-1/8″	

3/4″	4″	

2-1/4″
2-1/8″	

3/4″	4″	
2-1/4″

1″	

2-1/2″	4″

Pitch Required	

5-1/2″		

1-7/8″	
3″	

1-1/8″	

1/2″	
Varies

1/2″	

Pitch Required	

L41 Closure	OL41 Offset Cleat	AL41 Angle Cleat	ZL41 “Z” Clip	Z41 “Z” Closure	R41 Ridge	R42 Vented Ridge	

1-3/4″
2-1/4″	
1-1/2″

5/16″	13/16″	

2-3/8″

5/8″	
2 1/8″
1-3/4″

2” Length	2 1/8″
Pitch Required	
2-1/8″
1-3/4″

2-1/8″
Pitch Required	

8-1/2″

Pitch Required	

9″
1-1/2″ 3″

Pitch Required	

12" or 16" Net Coverage

12", 16", 17", or 18" Net Coverage