Not all colors and profiles are available at all locations. Please see back of color card for details.

STANDARD COLORS

We recommend you request a physical sample to review before ordering. We are not responsible for color variations.

				

ZINCALUME® Plus*
SRI: 64 • LRV: 67

CASCADE GRAY
SRI: 58 • LRV: 41

MATTE BLACK
SRI: N/A • LRV: 5

WEATHERED COPPER
SRI: 32 • LRV: 11

WINTER WHITE
SRI: 88 • LRV: 74

TAUPE
SRI: 53 • LRV: 28

CANYON RED
SRI: 45 • LRV: 16

SLATE GRAY
SRI: 32 • LRV: 13

SURF WHITE
SRI: 74 • LRV: 59

PATINA STEEL
SRI: 38 • LRV: 17

RUSTIC RED
SRI: 43 • LRV: 13

TAHOE BLUE
SRI: 33 • LRV: 14

LIGHT STONE
SRI: 70 • LRV: 53

CHESTNUT BROWN
SRI: 36 • LRV: 12

OLD TOWN GRAY
SRI: 43 • LRV: 27

EVERGLADE
SRI: 35 • LRV: 19

DESERT BEIGE
SRI: 58 • LRV: 39

CLASSIC BROWN
SRI: 29 • LRV: 7

OLD ZINC GRAY
SRI: 43 • LRV: 22

DENALI GREEN
SRI: 29 • LRV: 11

	

FOREST GREEN
SRI: 36 • LRV: 8

PREMIUM COLOR

NATURAL RUST1
SRI: 32 • LRV: 10
(Subject to upcharge)

COPPER PENNY1

MEASURED ON A SCALE OF 0 - 100
Light Reflective Value (LRV)
Measures how much visible light a color reflects and how much it absorbs. The higher the LRV, the more reflective it will be.

Solar Reflective Index (SRI)

Measures the amount of heat reflected from painted metal roof. The higher the SRI value, the cooler the metal will be, helping cut down on energy costs to keep your home cool.

IRONOX2
SRI: N/A • LRV: N/A

SRI: 53 • LRV: 28

SRI values in accordance with ASTM E1980 and are based on independent testing. Cool Roof Rating Council (CRRC) performance values (for CA Title 24) are based on color families and will differ from above.
SRI=Solar Reflective Index.  LRV=Light Reflectance Value.  GA= Gauge of Steel.  *Clear acrylic coated.

COLOR CHART

®

Customer Service Centers
Salem, OR: 503-390-7174 or 800-272-7023 I Spokane, WA: 509-536-4097 or 800-776-8771

www.ascbp.com

1 Please note, these colors are batch sensitive (may have color variation) and are directional in nature. Different batches are not to be mixed on projects.
2IronOx is black steel (uncoated and unpainted), that rusts naturally. No warranty is offered or implied. Only available in 22 GA Nu-Wave® Corrugated.
REPRESENTATION OF COLORS MAY VARY DUE TO PRINTING LIMITATIONS.
Sample color chips are available upon request. Consult your ASC Building Products representative for more information.

Color Key															36" Nu-Wave® Corrugated	
Dura Tech™ xl (SMP)	12" Skyline Roofing®	16" Skyline Roofing®														
ColorGuard 25 with Spectrascape® (Polyester)			
21⁄2" Corrugated						36" Strata Rib®			36" Delta Rib™ III				
Dura Tech™ nt (SMP)				
24" Delta Rib™		36" Nor-Clad®								36" PBR Panel		
ZINCALUME® Plus (Unpainted product)																
Premium Color (Subject to upcharge)																
Colors & Gauges	26	26	29	26	29	26	29	26	29	26	29	26	26	 26 	
ZINCALUME® Plus			AK/CA
OR/WA		1	WA		AK/CA
OR/WA		AK/CA
OR/WA						
Winter White			CA
OR/WA					AK/CA
OR/WA	OR
WA		AK/CA
OR/WA	WA							
Surf White								OR
WA			OR
WA								
Light Stone			CA
OR/WA					AK	CA
OR/WA		AK	CA							
												OR/WA							
Desert Beige								AK/CA
OR/WA	OR
WA		AK/CA
OR/WA	WA							
Cascade Gray								OR			OR								
Taupe								CA
OR/WA			CA
OR/WA								
Patina Steel			CA
OR/WA					CA
OR/WA			CA
OR/WA								
Chestnut Brown			AK/CA
OR/WA					AK/CA
OR/WA	OR
WA		AK/CA
OR/WA	WA							
Classic Brown			AK/CA
OR/WA					AK/CA
OR/WA			AK/CA
OR/WA								
Matte Black			AK/CA
OR/WA					AK/CA
OR/WA			AK/CA
OR/WA								
Canyon Red								AK/CA
OR/WA			AK/CA
OR/WA								
Rustic Red			AK/CA
OR/WA					AK/CA
OR/WA	OR
WA		AK/CA
OR/WA	WA							
Old Town Gray			CA
OR/WA					AK/CA
OR/WA	OR
WA		AK/CA
OR/WA	WA							
Old Zinc Gray			AK/CA
OR/WA					AK/CA
OR/WA			AK/CA
OR/WA								
Weathered Copper			AK/CA
OR/WA					AK/CA
OR/WA			AK/CA
OR/WA								
Slate Gray			AK/CA
OR/WA			CA		AK/CA
OR/WA			AK/CA
OR/WA								
Tahoe Blue			AK/CA
OR/WA			WA		AK/CA
OR/WA		OR	AK/CA
OR/WA		OR						
Everglade			CA
OR/WA					AK/CA
OR/WA			AK/CA
OR/WA								
Denali Green			AK/CA
OR/WA					AK/CA
OR/WA	OR
WA		AK/CA
OR/WA	WA							
Forest Green			AK/CA
OR/WA					AK/CA
OR/WA	OR
WA		AK/CA
OR/WA	WA							
Copper Penny*			AK/CA
OR/WA					AK/CA
OR/WA			AK/CA
OR/WA								
Natural Rust*			AK/CA
OR/WA	1				AK
WA		AK
WA							
IronOx2																2	

Production Locations

Salem, OR.

Multiple Locations (See Key)

Sacramento, CA. Sacramento, CA.
Sacramento, CA., Spokane, WA.
Sacramento, CA.

Multiple Locations (See key)

Sacramento, CA., Salem, OR.

Multiple Locations (See key)

Sacramento, CA., Salem, OR.

Salem, OR.

Sacramento, CA.

Sacramento, CA.

Anchorage, Alaska (AK) Sacramento, California (CA) Salem, Oregon (OR) Spokane, Washington (WA)

FOOTNOTES:
Also available in 32" Net Coverage.
IronOx is black steel (uncoated and unpainted), that rusts naturally. No warranty is offered or implied. Only available in 22 GA Nu-Wave®
Corrugated.
Dura Tech™ 5000/mx (PVDF) 24ga & 22ga colors available for:
Skyline Roofing hp, Nu-Wave Corrugated, PBR Panel, and Design Span hp.
See ascbp.com for Dura Tech™ 5000/mx color chart.

* Please note these colors are batch sensitive (may have color variation) and are directional in nature. Different batches are not to be mixed on projects. We recommend you request a sample of current stocked material to review actual color before ordering to ensure color accuracy.
WE ARE NOT RESPONSIBLE FOR COLOR VARIATIONS.

FINISHES DEVELOPED BY

PRODUCT DETAILS AND SPECS

®

All information stated in the color card is correct at time of printing and subject to change without notice.
©2008-2024 ASC Profiles LLC All rights reserved. Spectrascape® is a registered trademark of Steelscape, LLC. ZINCALUME® is a registered trademark of BlueScope Steel Ltd. 0224 web (CC150)

www.ascbp.com