FLASH X/Y
Cuslom Flashing • Girth Computation
LineComment Format	Girth	SAC	ANC SPO	SLC	SLM	#
Strokes	
XYZFm ringNa,re
PIOCIUd C OCI&
tinec	t Format							
FCB_B& FCB_P
1 HEM
·2 HEMS
2_GABARE or COLOR, PART DESCRIPTION OR DRAWING#	Add leg dimensions+ hems as:	
.5
1	
.375
.75	
.4375
.875	
.375
.875		
Custom Eave EAVXY_B &EAVXY_P
X=  =Y	:12 PITCH COLOR (If PTO M)	
X+Y+	
.5	
.5	
.5	
.5	
3	
Custom Eave with Hemmed Drip Edge EAVHXY_B &EAVHXY_P
X=  =Y	:12 PITCH COLOR (If PTO Ml	
X+Y+	
1	
.875	
.9375	
.875	
5	
Custom L Fl ashin g FLASHXY_B & FLASHXY_P
X=  =Y	DEG COLOR (If PTO M) IN or OUT	
X+Y					
2	
Custom WidthFlat Sheet FSX_B & FSX_P
X=  COLOR (If PTO M)	
X					
2	
Custom Gable GABXY_B &GABXY_P X=  =Y  COLOR (If PTO M)	
X+Y+	
3.375	
3.125	
3.25	
3.25	
9	
Custom SkylineGable SKGABXY_B & SKGABXY_P
X=  =Y  COLOR	
X+Y+	
3.375	
6.125	
3.25	
3.25	
9	
Custom Single Hem Open Jamb JAMSH_B & JAMSH_P
X=  =Y  COLOR (If PTO M)	
X+Y+	
.5	
.375	
.4375	
.375	
4	
Custom DoubleHem Open Jamb JAMDH_B & JAMDH_P
X=  =Y  COLOR (If PTO M)	
X+Y+	
1	
.75	
.875	
.875	
6	
Custom ClosedJamb JAMXYZ_B & JAMXYZ_P
X=  =Y  Z= COLOR (If PTO Ml	
X+ Y + Z	NA				
3	
Custom DoubleHem Cl osed Jamb JAMDHXYZ_B &JAMDHXYZ_P
X=  =Y  Z= COLOR (If PTO M)	
X + Y + Z +	NA	NA	NA	
.875	
7	
Custom OutsideCorner
OSCXY_B &OSCXY_P X=  =Y  COLOR (If PTO M)	
X+Y+	
4.5	
4.25	
4.375	
4.375	
10	
Custom Standard Ridge RIDCS_B & RIDCS_P
X=	:12 PITCH COLOR (If PTO M)	
X+Y+	
1	
.75	
.875	
.875	
6	
Custom VentedRidge RIDCV_B& RIDCV_P
X=	:12 PITCH COLOR (If PTO M)	
X+Y+	7.25	
7	
7.125	
7.125	
10	
Custom Zee Tri m
ZXYZ_B & ZXYZ_P
X=  =Y  Z= COLOR (If PTO M)	
X+ Y + Z					
3