Flex Series
(Horizontal Installation) Installation Guide

Flex Series
(Horizontal Install.) Installation Guide

Table of Contents -

Section	Page

General Notes . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . .	i
Panel Details	1
Clips	2
Panel Closures	3
Closure Installation	4
Base	5
Sill	6
End Wall . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . .	7
Outside Corner . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . .	8
Inside Corner	9
Soffit (Front)	10
Soffit (Back)	11
End Splice (w/Trim)	12
Parapet	13
Door/Window (Head)	14
Door/Window (Jamb)	15
Door/Window (Sill)	16
Wall Penetration (3D)	17
Wall Penetration	18
Rigid Insulation	19

©2018 ASC Profiles.  All rights reserved.	Nov18

General Notes
The attached installation details are intended to be a design aid and do not depict all situations. Modifications are the responsibility of the designer/user and should take into account climate conditions such as wind and snow, governing code requirements, and the actual usage and maintenance of the structure.

Applications:
Flex Series can be utilized as a wall panel installed in the vertical or horizontal orientation. It shall not be utilized for roof applications. Flex Series can be used over solid substrates or over spaced supports. This installation guide depicts clip attached panels installed using flush mounted clips. Details for direct fastened panels or clip attached panels using standoff clips would be similar.

Flashings:
Where possible, flashings should be lapped away from prevailing winds. Certain flashings should be supported if it is likely that equipment (ladder, etc.) will be used against them. Check with AEP Span any time you intend to specify a prefinished flashing in a gauge or finish different than the Flex Series. It is good practice to specify that all flashings be of the same material (gauge, color, finish) as the roof panels to ensure long-term durability. Field-painted flashings rarely equal the durability and colorfastness of factory baked-on paint systems. The enclosed details have minimized the use of exposed fasteners where possible. The edges of flashings have also been shown hemmed to strengthen and to minimize the exposure of cut edges.

Flashing design and fabrication is generally the responsibility of the contractor. For convenience, we have provided some typical flashing drawings on our website at http://www.aepspan.com/roof/prodDetailad08.ht ml?id=35 . Applicable Flex Series flashing part numbers are referenced within this installation guide. Note that flashing shapes and dimensions may vary greatly based on project requirements. Installation details and flashings referenced within are for general design guidance only.

Condensation, Insulation, & Ventilation:
It is the designer's responsibility to determine the need and composition of condensation control materials including insulation and vapor retarders, as well as ventilation requirements.
Metal wall products are susceptible to condensation and its control should be carefully considered.

Thermal Movement:
Both panels and flashings must allow for thermal movement (expansion and contraction) of the materials, especially where long lengths are used. Appropriate gaps or provisions must be provided to accommodate thermal movement.

Oil Canning:
Flat metal surfaces often display waviness commonly referred to as 'oil canning'. This can be caused by variations in raw material, processing variations, product handling, or variations in the installation substrate. Oil canning is a characteristic, not a defect, of panels manufactured from light-gauge metal. To reduce potential for oil canning, substrates should not deviate from a flat plane more than 1/4 inch in 20 feet, or 1/8 inch in 5 feet. Oil canning is not a cause for panel rejection. Additional technical information is available upon request.

References:
The Sheet Metal and Air Conditioning Contractors' National Association Inc. (SMACNA) manual is an excellent reference for sheet metal contractors. It’s guidelines for underlayments, gutter and downspout size requirements, and expansion/contraction of metals and flashing joints should be followed.

Technical Assistance:
Contact your AEP Span Sales Representative for additional information.

i

r	I--	---1	---1	12"
2
L.	2"-	"
1.2FX10-12	,1r-
Ll
1.2FX20-12	1¾,"&-
1.5FX20-12	1r

Lr
1.2FX30-12	1f,'&-
1.5FX30-12	1r

1.2FX40-12
1.5FX40-12

PANEL INTERLOCK	l 	
OPTIONS

DIRECT FASTENED ('D' P/N SUFFIX)

MATERIAL:
STEEL: 22 & 24GA (20GA NON-STD.) AVAILABLE LENGTHS: 5' -20'	

COVERAGE

1		

CLIP ATTACHED ('C' P/N SUFFIX)	-
'I --,		

N
I...	FLEX SERIES
HORIZONTAL INSTALL.	
PANEL DETAILS	
		indvi	FXH-01	

..)	

-- 	12"	COVERAGE	-
1O"	7
'	
	I --,	

-- 		12"	COVERAGE	-
6"	1
'	
	I --,	

-- 	  	
4"	l	12"	COVERAGE
2"I	4"	-	
			I --,	

			

9/32" DIA		

I
i	0
I
I
rrj--½	)2J)
0
0
r-(t	)25)
I I
i	0
I	 	

 STANDOFF CLIP
P/ N: #WALLCL PO. 5

 				

3"	
):,	D
0		t
7/8"
t
9/16"					
	0
):,	D		t					

L_	0
L	2 1/ 2"	J						

 FLUSH CLIP							
	P/ N: #WALLCLP							

rr							
	
 				2	t
1/2"
GAP
T				
			
 INSTALLED 	
POSITION				

N
I...	FLEX SERIES
HORIZONTAL INSTALL.	
CLIPS	
		indeH	FXH-02	

.)	

r

TOP SIDE CLOSURE FOR ALL PANELS &
CL1.2FX-1P	BOTTOM SIDE CLOSURE FOR 1 . 2FX 10-12
& 1.2FX3O- 12

CL1.2FX-2P	M  SIDE  CLOSURE  FOR
FX2O-12  &  1.2FX40-12

FOR PANEL HEM

TEAROFF PERFORATED PLUG SECTIONS TO FILL PANEL REVEALS AS REQUIRED

TOP SIDE CLOSURE FOR ALL PANELS.
CL1.5FX-1P	BOTTOM SIDE CLOSURE FOR 1.5FX1O-12
& 1.5FX3O-1 2

CL1.5F X- 2 P	M  SIDE  CLOSURE FOR
5FX20-12   &   1. 5 FX4O- 12

NOTE:	APPLICATIONS UTILIZING STANDOFF CLIP ALSO REQUIRE UNIVERSAL CLOSURE STRIP (AEP #CLEM1x19 . 68 OR EQUIV.) TO SEAL OFF ADDITIONAL 1/2" PANEL-TO-SUBSTRATE GAP.	

N
I...	FLEX SERIES
HORIZONTAL INSTALL.	
PANEL CLOSURES	
		indvi	FXH-03
.)	

r
OPTIONAL: 1"W x 1/8"THK FOAM TAPE (MAS .125PE) TO SECURE CLOSURE PLUGS

TOP SIDE CLOSURE INSTALLATION

TOP CLOSURE
PLUG
SEALANT BE

BOTTOM SIDE CLOSURE INSTALLATION
(FLUSH MOUNTED PANELS)

BOTTOM SIDE CLOSURE INSTALLATION
(PANELS WITH STANDOFF CU

BOTTOM CLOSURE PLUG

1X1 UNIVERSAL CLOSURE STRIP (AEP  #CLEM1X19.68
OR EQUIV.)

NOTES:
- ALL CLOSURE PLUGS SECURED AND SEALED WITH POLYURETHANE SEALANT
(X) - NOT BY AEP SPAN	

N
I...	FLEX SERIES
HORIZONTAL INSTALL.	
CLOSURE INSTALLATION	
		indvi	FXH-04
..)	

r

TRIM	DIM  A	USAGE
ZC226	1  1/4"	1. 2FX FLUSH MOUNT ZC22O	1 3/4"	1.2FX W/O.5" STANDOFF
1  1/2"	ZC224	1 1/2"	1.5FX FLUSH MOUNT
A	ZC227	2"	1. 5FX W/ O. 5" STANDOFF

1 1/2"

TRIM	DIM  A	USAGE
4"	DFO22	1  5/8"	1. 2FX FLUSH MOUNT
DFO23	2 1/8"	1. 2FX W/ O. 5" STANDOFF
DFO24	1   7/8"	1. 5FX FLUSH MOUNT DFO25	2 3/ 8"    1. 5FX  W/ O. 5"  STANDOFF
1''	A
1/2"
135·

SUBSTRATE

SPECIFIED UNDERLA YMENT (X)

BUTYL FLASHING TAPE (MAS.O25BF)

1 / 8 " THK HORSESHOE SHIM (SHIM.125) OR EQUIVALENT - SEE NOTE 1

Z-METAL

TRIM FASTENER OR RIVET AT 12" O. C. MAXIMUM

DRIP FLASHING

 		p

1. SHIM USED FOR MOISTURE CONTROL
(DRAINAGE)   IN  FLUSH  MOUNT  APPLICATIONS.	FLEX SERIES PANELS ARE INSTALLED
(X)    -    NOT   BY AEP  SPAN	FROM GROUND TO EAVE.	

N
I...	FLEX SERIES
HORIZONTAL INSTALL.

BASE	
		indvi	FXH-05
..)	

r

TRIM	DIM  A	USAGE
ZC226	1  1/4"	1.2FX FLUSH MOUNT ZC22O	1  3/4"	1.2FX W/O.5" STANDOFF
1  1/ 2 "	ZC224	1 1/2"	1.5FX FLUSH MOUNT
A	ZC227	2"	1.5FX W/O.5" STANDOFF

1 1/2"

.   .·  . 1
. ,    I
,     •     I
. .. ·1
• I
•• I

.     ..·     1	SUBSTRATE
• I
••	I	SPECIFIED UNDERLA YMENT (X)
. .. · 1
'.	I	BUTYL FLASHING TAPE (MAS.O25BF)
. J,11,

1/8"	THK HORSESHOE SHIM (SHIM.125)
••    I	OR EQUIVALENT - SEE NOTE 1
••	I
.  .  ·.    1
Z-METAL
••	I
••       I
.    .·    . 1	TRIM FASTENER OR RIVET
• I	AT  12"   O.C.  MAXIMUM
•   I
. .  .·1	SILL  FLASHING  (V)
. • I
ALTERNATE WALL MATERIALS
.     ..·     1

• I
••	I
. J	 	1/ 4'	GAP
t

1. SHIM USED FOR MOISTURE CONTROL (DRAINAGE) IN FLUSH MOUNT APP LICATIONS.
(X) - NOT BY AEP SPAN
(V) - DIMENSIONS VARY BASED ON PROJECT CONDITIONS	

N
I...	FLEX SERIES
HORIZONTAL INSTALL.

SILL	
		indvi	FXH-06
.)	

r

3"	TRIM	DIM  A	USAGE
JT1O9	1  1/2"	1.2FX FLUSH MOUNT
A		JT11O	2"	1.2FX W/O.5" STANDOFF 1/2"	JT1O7	1  3/4"	1.5FX FLUSH MOUNT
JT111	2  1/4"	1.5FX W/O.5" STANDOFF
1 1/2"

.  4
CLIP FASTENER
<1
PANEL CLIP

SPECIFIED UNDERLA YMENT (X)

4	<1.	SUBSTRATE
,:I

. "
l
 		-ry::J i • · • · • · • · • · • · • · • · • · • · • · • · • · •
. <1

4

. <1

4

<1	OPTIONAL FIELD FABRICATED
CLOSURE COVER TRIM (X)
. 4
OUTSIDE CLOSURE (SEALED &
SECURED WITH SEALANT)

CONTINUOUS BEAD OF  NON­ SKINNING BUTYL TAPE OR SEALANT

TRIM FASTENER W/SEALING WASHER OR RIVET AT 12" O.C. MAXIMUM

J TRIM

SEALANT/ BACKER ROD

(X) - NOT BY AEP SPAN	

N	FLEX SERIES
HORIZONTAL INSTALL.	
END WALL	
		indvi	FXH-07
.)	

r

1/2"

4"
. I
.  ·I,
.

1/2"

4"
OC111

CLIP FASTENER

PANEL CLIP SUBSTRATE
SPECIFIED UNDERLA YMENT (X)

OPTIONAL FIELD FORMED CLOSURE  COVER  TRIM (X)

OUTSIDE  CLOSURE  (SEALED  &
SECURED  WITH SEALANT)

CONTINUOUS BEAD OF NON­ SKINNING  BUTYL  TAPE  OR  SEALANT

TRIM FASTENER W/SEALING WASHER OR RIVET AT 12" O. C. MAXIMUM

OUTSIDE  CORNER  TRIM (OC111)

(X) - NOT BY AEP SPAN	

N
I...	FLEX SERIES
HORIZONTAL INSTALL.

OUTSIDE CORNER	
		indvi	FXH-08
.)	

r

1/2"

4"

4"

1 /2"  l	IC093

·:.::.:r -. • .·• -.-... .,-..-.. .. -.. . i=.v=-.. . .- . . 1-  	1
 	,          ..	I
. -I
>> I
. -I
• I
. . . ·1	SUBSTRATE
..	I
. -    1
--1	SPECIFIED UNDERLA YMENT (X)
INSIDE CORNER TRIM (ICO93)
I

TRIM FASTENER W/SEALING WASHER RIVET AT 12" O. C. MAXIMUM

CONTINUOUS BEAD OF  NON­ SKINNING BUTYL TAPE OR SEALANT

OUTSIDE CLOSURE (SEALED &
SECURED  WITH SEALANT)

OPTIONAL FIELD FORMED CLOSURE  COVER  TRIM (X)

PANEL CLIP CLIP FASTENER

(X) - NOT BY AEP SPAN	

  	N
I...	FLEX SERIES
HORIZONTAL INSTALL.

INSIDE CORNER	
		indvi	FXH-09
..)	

r
TRIM	DIM  A	USAGE	TRIM	DIM  A	USAGE
ZC226	1  1/4"	1. 2FX FLUSH MOUNT	DFO28	1  1/2"	1. 2FX FLUSH MOUNT
ZC220	1 3/4"	1. 2FX W/ O. 5" STANDOFF
1  1/2"	ZC224	1 1/2"	1. 5FX FLUSH MOUNT	DFO29	2"	1.2FX W/ O. 5" STANDOFF
A	ZC227	2"	1. 5FX W/O.5" STANDOFF	4"	DFO30	1  3/4"	1.5FX FLUSH MOUNT
DFO31	2 1/4"	1. 5FX W/ O. 5" STANDOFF

1 1/2"
135°  A

1/2"
(V)	1/ 2 "	OPEN HEM
1/2"
135·

COVER TRIM

CLIP FASTENER PANEL CLIP SUBSTRATE
SPECIFIED UNDERLA YMENT (X)

BUTYL  FLASHING  TAPE
(MAS . 025BF)

1 /8"	THK HORSESHOE SHIM (SHIM .125)   OR EQUIVALENT
SEE NOTE 1 Z-METAL
TRIM  FASTENER  OR RIVET
AT  12"   O. C. MAXIMUM

DRIP  FLASHING)
 	·.    j.·..:     . . ·. . ·. . ·. . ·. . ·. . ·. . ·. . ·. . ·. . ·.

1/ 4'	 	

OPTIONAL FIELD FABRICATED CLOSURE COVER TRIM (X)

OUTSIDE CLOSURE (SEALED &
SECURED WITH SEALANT)

CONTINUOUS BEAD OF  NON­ SKINNING  BUTYL  TAPE  OR  SEALANT
TRIM  FASTENER  W/SEALING WASHER
1.  SHIM  USED  FOR  MOISTURE  CO	OR RIVET AT 12" O. C. MAXIMUM MOUNT APPLICATIONS.
(X)    -    NOT   BY AEP  SPAN	COVER TRIM (V)
(V) - DIMENSIONS VARY BASED ON PROJECT CONDITIONS	

N
I...	FLEX SERIES
HORIZONTAL INSTALL.	
SOFFIT (FRONT)	
		indvi	FXH-10
..)	

r

1/2"

4"

4"

1/2"

ij 	
· .  ·.   .  ·.   .  ·.   .  j._. J·. _·.   .  ·.   .. ·.  ·	
7 ....
1· .
I           ••
I
\\\;;,.
1 ·

OPTIONAL  FIELD  FABRICATED	..
CLOSURE  COVER  TRIM (X)	I ..
I .
OUTSIDE  CLOSURE  (SE	1·..
SECURED   WITH  S	I..
1·  I      .
INSIDE CORNER TRIM
-   1··
I            .
SPECIFIED  UNDERLA YM	1 · ..
I. .
SUB	1· .
TRIM FASTENER W/SEALING WASHER OR RIVET AT 12 " O.C. MAXIMUM

CONTINUOUS BEAD OF NON­ SKINNING  BUTYL  TAPE  OR  SEALANT

CLIP FASTENER PANEL  CLIP

(X) - NOT BY AEP SPAN	

N
I...	FLEX SERIES
HORIZONTAL INSTALL.	
SOFFIT (BACK)	
		indvi	FXH-11
.)	

r
3"	TRIM	DIM  A	USAGE
MT111	1  1/2"	1.2FX  FLUSH MOUNT
A		MT112	2"	1.2FX W/O.5" STANDOFF 1  1/2"	1/2"	MT109	1  3 / 4"	1. 5FX FLUSH MOUNT
MT113	2   1/4"	1. 5FX W/ O. 5" STANDOFF
3"

CLIP FASTENER PANEL CLIP SUBSTRATE
SPECIFIED UNDERLA YMENT (X)

. ..   ...   . ·.   .-it .  .   . · . ....	.	.

OPTIONAL FIELD FABRICATED CLOSURE COVER TRIM (X)
3"	OUTSIDE CLOSURE (SEALED &
SECURED WITH SEALANT)
A
1/2"
CONTINUOUS BEAD OF NON­
1  1/2"	SKINNING BUTYL  TAPE OR SEALANT
TRIM	DIM  A	USAGE	TRIM  FASTENER  W/SEALING WASHER
JT1O9	1  1/  2 "	1. 2FX FLUSH  MOUNT	OR RIVET AT 12 " O. C. MAXIMUM JT11O	2"	1. 2FX W/ O. 5" STANDOFF
JT107	1   3/4"	1. 5FX FLUSH MOUNT
JT111	2 1/4"	1. 5FX W/ O. 5"  STANDOFF	END SPLICE

REVEAL FLASHING (V)

 		.	Q	.	.   Q   . -	.	. · . ·.·1.	. · . · . · .
¾-	 	1	------

JTRIM

(X) - NOT BY AEP SPAN
(V) - DIMENSIONS VARY BASED ON PROJECT CONDITIONS	

N
I...	FLEX SERIES
HORIZONTAL INSTALL.	
END SPLICE (W/TRIM)	
		indvi	FXH-12
..)	

r

1  1/2"

135'
5/8"

TC2O9

1/4:12 MIN. SLOPE

PARAPET FLASHING (V) BLOCKING  (AS  REQUIRED)
TRIM   CLEAT (TC2O9)

TRIM FASTENER W/SEALING WASHER OR RIVET AT 12" O.C. MAXIMUM

CONTINUOUS BEAD OF NON­ SKINNING  BUTYL  TAPE  OR  SEALANT

SPECIFIED UNDERLA YMENT (X)

SUBSTRATE CLIP FASTENER PANEL CLIP

(X) - NOT BY AEP SPAN
(V) - DIMENSIONS VARY BASED ON PROJECT CONDITIONS	

N
I...	FLEX SERIES
HORIZONTAL INSTALL.	
PARAPET	
		indvi	FXH-13
..)	

r

TRIM	DIM  A	USAGE	1 1/2" HT095	1  1/2"	1. 2FX FLUSH MOUNT		A
4"	HT100	2"	1. 2FX W/0.5" STANDOFF
HT091	1  3 / 4"	1. SFX FLUSH  MOUNT
HT101	2  1/ 4 "	1. SFX W/0.5"  STANDOFF	1 1/2"

A	1/2"	TRIM	DIM  A	USAGE
1/2"
135'	4"	135'	ZC226	1  1/ 4 "	1.2FX FLUSH MOUNT
ZC220	1  3/4"	1. 2FX W/ 0 . 5" STANDOFF ZC224	1 1/2"	1. 5FX FLUSH MOUNT ZC227	2"	1. 5FX W/ 0 . 5" STANDOFF

I·	1n	I
-:    : !      IJL_J
I         .	I
I	I
I  ..  I
I   . ·'

SUBSTRATE

SPECIFIED UNDERLA YMENT  (X) BUTYL FLASHING TAPE (MAS .0 25BF)
1/8"	THK HORSESHOE SHIM (SHIM .125) OR EQUIVALENT - SEE NOTE 1

Z-METAL

TRIM FASTENER OR RIVET AT 12" O.C. MAXIMUM

HEADER TRIM

1. SHIM USED FOR MOISTURE CONTROL (DRAINAGE) IN FLUSH MOUNT APPLICATIONS.
(X) - NOT BY AEP SPAN	

I...	FLEX SERIES
HORIZONTAL INSTALL.

	DOOR / WINDOW (HEAD)	
		indvi	FXH-14
..)	

r
135'	/	--------
1/2"

/
I	SEALANT
/

I	TRIM ANGLE
4"	I
WALL CLOSURE

1/2"
1 1/2" WC217
 ALTERNATE DETAIL

CLIP FASTENER	r 	

PANEL CLIP SUBSTRATE
SPECIFIED
UNDERLA YMENT  (X)	]

OPTIONAL FIELD FABRICATED CLOSURE COVER TRIM (X)

OUTSIDE  CLOSURE  (SEALED  &
SECURED  WITH SEALANT)

CONTINUOUS BEAD OF NON­ SKINNING  BUTYL  TAPE  OR  SEALANT

TRIM FASTENER W/SEALING WASHER OR RIVET AT 12" O.C. MAXIMUM

WALL  CLOSURE  (WC217)

(X) - NOT BY AEP SPAN	

I...	FLEX SERIES
HORIZONTAL INSTALL.	DOOR / WINDOW (JAMB)	
		indvi	FXH-15
.)	

r

1/2"
TRIM	DIM  A	USAGE	135·
1  1/2"	ZC226	1  1/4"	1. 2FX FLUSH MOUNT
A	ZC22O	1 3/4"	1. 2FX W/ O.5 " STANDOFF ZC224	1 1/2"	1. SFX FLUSH MOUNT
ZC227	2"	1. SFX W/ O. 5 "  STANDOFF	4"
1 1/2"

1/2"

1 1/2" WC217

•  I
.                  ·   1
WALL CLOSURE (WC217)

.       · 1
TRIM FASTENER W/SEALING WASHER
. .. · 1	OR RIVET AT 12" O.C. MAXIMUM
• I
CONTINUOUS BEAD OF  NON­ SKINNING BUTYL TAPE OR SEALANT

• I
. . .·1	Z-METAL
•  I	SUBSTRATE
.                   ·   1
.      ..·        1	SPECIFIED UNDERLA YMENT  (X)
.                     ·    1
••                  I
CLIP FASTENER
i i	PANEL CLIP
I
I
..     I
.    .  I
.                   ·   1
.. .. I
<< j7

(X)	-	NOT BY AEP SPAN	

N
I...	FLEX SERIES
HORIZONTAL INSTALL.

	DOOR / WINDOW (SILL)	
		indvi	FXH-16
..)	

r

TRIM  FASTENER W/SEALING
WASHER,  OR RIVET
SEALANT OVERLAP UPPER/LOWER
FLASHINGS

WALL  PENETRATION

>	SEAL PERIMETER OF FLASHINGS AND ALL TRIM OVERLAPS WITH A
CONTINUOUS BEAD OF NON­ SKINNING BUTYL TAPE OR SEALANT

OPTIONAL FIELD FABRICATED CLOSURE COVER TRIM (X)

OUTSIDE CLOSURE (SEALED &
SECURED WITH SEALANT)

l	LOWER VIEW
I
(X) - NOT BY AEP SPAN	

N
I...	FLEX SERIES
HORIZONTAL INSTALL.	
WALL PENETRATION (3D)	
		indvi	FXH-17
.)	
REV. 6/19/17

r

I I I I I I
SPECIFIED	II..•..•  I
UNDERLA YMENT (X)	.   .    I
I,_-_-   I
I
SUBSTRATE	I         •    • I
TRIM FASTENER W/SEALING	T-------------
WASHER  OR RIVET

CONTINUOUS BEAD OF NON­ SKINNING BUTYL TAPE OR SEALANT UNDER COVER PERIMETER

SEAL PENETRATION PERIMETER WITH  POLYURETHANE SEALANT

WALL  PENETRATION
OVERLAPPED PENETRATION COVER	-r--
1
OPTIONAL  FIELD  FABRICATED	I
CLOSURE  COVER  TRIM  (X)	I
I
OUTSIDE   CLOSURE (SEALED  &	I
SECURED  WITH  SEALANT)	I
I
I
PROVIDE  SUFFICIENT  CLEARANCE	I
BETWEEN FLASHING & PENETRATION TO ACCOMODATE THERMAL MOVEMENT .

(X) - NOT BY AEP SPAN	

N
I...	FLEX SERIES
HORIZONTAL INSTALL.	
WALL PENETRATION	
		indvi	FXH-18
..)	

r

.·      .·       1
. . I

.

.  I

SUBSTRATE RIGID  INSULATION (X)
SPECIFIED
UNDERLA YMENT (X)

ZEE  FLASHING (V)

SUBGIRT CLIP FASTENER PANEL CLIP

(X) - NOT BY AEP SPAN
(V) - DIMENSIONS AND GAGE VARY BASED ON PROJECT CONDITIONS

FLEX SERIES
HORIZONTAL INSTALL.	RIGID INSULATION

N
I...

indvi	FXH-19

..)

MANUFACTURING FACILITY:

Tacoma, Washington
2141 Milwaukee Way
Tacoma, WA 98421

Fontana, California
10905 Beech Avenue
Fontana, CA 92337

CORPORATE HEADQUARTERS:

ASC Profiles LLC 2110 Enterprise Boulevard West Sacramento, CA 95691

CUSTOMER SERVICE:
800-733-4955

Visit us at:
www.aepspan.com

©2018 ASC Profiles LLC.  All rights reserved.