®

Nu-Wave® Corrugated & IronOx Corrugated Siding
Installation Guide

Table of Contents

General
Notes	i - ii
Panel details	1

Fasteners	2

Roof Installation Details
Eave	4
Eave with Gutter	5
Gutter, Post-Hung	6
Gable	7
Valley	8
Ridge	9
Vented Ridge	10
Peak	11

Sidewall	12
Endwall	13
Slope Transition - High to Low	14
Slope Transition - Low to High	15
Panel Lap	16
Roof Curb	17
Curb Flashings	18

Vertical Wall Installation Details
Base	20
Sill	21
Endwall	22
Outside Corner	23
Inside Corner	24
Soffit, Front	25
Soffit, Back	26
Parapet	27
Door / Window (Head)	28

Opening, Head (Nail Fin)	29
Door / Window (Jamb)	30
Opening, Jamb (Nail Fin)	31
Door / Window (Sill)	32
Opening, Sill (Nail Fin)	33
Penetration, 3D	34
Penetration, 2D	35
Penetration Examples	36

Horizontal Wall Installation Details
Base	38
Sill	39
Eave / Fascia	40
Endwall	41
Outside Corner	42
Inside Corner	43
Soffit, Front	44
Soffit, Back	45
Parapet	46

Door / Window (Head)	47
Opening, Head (Nail Fin)	48
Door / Window (Jamb)	49
Opening, Jamb (Nail Fin)	50
Door / Window (Sill)	51
Opening, Sill (Nail Fin)	52
Penetration, 3D	53
Penetration, 2D	54
Penetration Examples	55

GENERAL NOTES

The attached installation details are intended to be a design aid and do not depict all situations.
Modifications are the responsibility of the designer/user and should consider climate conditions such as wind and snow, wildfire, governing code requirements, and the actual usage and maintenance of the structure.

Flashing design and fabrication is generally the responsibility of the contractor. For convenience, we have provided typical flashing drawings on our website. Applicable Nu-Wave flashing part numbers are referenced within this installation guide. Note that flashing shapes and dimensions may vary greatly based on project requirements. Installation details and flashings referenced within are for general design guidance only.

Applications:
Nu-Wave is acceptable for use as a roofing panel and as a wall panel installed in the vertical or horizontal orientation. The recommended minimum slope is 3:12. Nu-Wave can be installed over solid substrates or over spaced supports. This installation guide depicts Nu-Wave installed over mixed substrates. It is the responsibility of the designer/user to make proper installation adjustments to address the installation conditions on the project.

Flashings:
Where feasible, flashings should be lapped away from prevailing winds. Certain flashings should be supported if it is likely that equipment (ladder, etc.) will be used against them. Check with ASC Building Products any time you intend to specify a prefinished flashing in a gauge or finish different than the
Nu-Wave panels. It is good practice to specify that all flashings be of the same material (gauge, color, finish) as the roof & wall panels to ensure long-term durability. Painted flashings rarely equal the durability and colorfastness of factory baked-on paint systems. The enclosed details have minimized the use of exposed fasteners where possible. The edges of flashings have also been shown hemmed to strengthen and to minimize the exposure of cut edges.

REV. 12/9/25

Condensation, Insulation, & Ventilation:
It is the designer's responsibility to determine the need and composition of moisture control materials including insulation and vapor retarders, as well as ventilation requirements. Metal roof and wall products are susceptible to condensation, and its control should be carefully considered.
For metal roofing panels, an underlayment should be installed over the roof substrate. ASC Building Products recommends using AEP Span Underlayment HT, which is specifically engineered for all ASC Building Products' roofing systems and suitable for use under any metal roofing system or coping. AEP Span Underlayment HT is a high-temperature,
self-healing, self-adhering, peel-and-stick underlayment with a non-abrasive surface that will not mar, scratch, or abrade the underside of metal panels and flashings. Please note that additional protection may be required to achieve Class A fire ratings as defined in UL 790 classified assemblies.

Thermal Movement:
Both panels and flashings must allow for thermal movement (expansion and contraction) of the materials, especially where long lengths are used. Appropriate gaps or provisions must be provided to accommodate thermal movement.

i

Designing for Snow:
If possible, valleys, gutters, roof elevation changes and penetrations should be minimized or eliminated in snow areas. Roof penetrations should be located as close to the ridge or peak of the roof as possible to minimize accumulations of ice and snow.

Building Code Compliance:
Nu-Wave is compliant with the IBC, IRC, CBC, and CRC building codes. Refer to IAPMO-UES Code Compliance Report #ER-0550 for further details. Nu-Wave is also approved as part of a Class A Fire rated assembly when installed in accordance to UL790 listings.

Panel Attachment / Structural Performance:
The structural performance of Nu-Wave is documented in IAPMO-UES Code Compliance Report #ER-0550. Published performance data includes: Panel section properties, inward (gravity) load capacities, outward (wind uplift) load capacities, shear tables, and other product information and limitations.

Protecting the Panels:
Proper handling, storage, installation, and keeping work surfaces clean are key to protecting metal roofing and siding. Regular washing and maintenance after installation further help ensure panel longevity. For detailed guidance, refer to the technical resources on ASC Building Products’ website.

References:
The Sheet Metal and Air Conditioning Contractors' National Association Inc. (SMACNA) manual is an excellent reference for sheet metal contractors. It's guidelines for underlayments, gutter and downspout size requirements, and expansion/contraction of metals and flashing joints should be followed.

Technical Assistance:
Contact your ASC Building Products' Sales Representative for additional information.

Nu-Wave Online Product Page:

Oil Canning:
Flat metal surfaces often display waviness commonly referred to as 'oil canning'. This can be caused by variations in raw material, processing variations, product handling, or variations in the installation substrate. Oil canning is a characteristic, not a defect, of panels manufactured from light-gauge metal. To reduce potential for oil canning, substrates should not deviate from a flat plane more than 1/4 inch in 20 feet, or 1/8 inch in 5 feet. Oil canning is not a cause for panel rejection. Additional technical information is available for review on our website.

Technical Resources:

ER-0550 Code Compliance Report:

REV. 12/9/25	ii

r
r	32'	COVERAGE	-

NU-WAVE CORRUGATED ROOF INSTALLATION (2 RIB LAP)

34-2/3'  COVERAGE

NU-WAVE CORRUGATED WALL INSTALLATION (1 RIB LAP)

PANEL FASTENER SPACING	RECOMMENDED LAP FASTENER
DEPENDENT UPON PROJECT	SPACING: 18" O.C. MAX.
STRUCTURAL REQUIREMENTS
•
�
32-5 ATTACHMENT PATTERN	34.7-5 ATTACHMENT PATTERN

	
32- 7 ATTACHMENT PATTERN	34.7- 7 ATTACHMENT PATTERN ROOF INSTALL		 WALL INSTALL
NOTE: PANEL FASTENER ATTACHMENT (TYPE, SIZE, AND LOCATION) IS DEPENDENT UPON
SUBSTRATE USAGE AND STRUCTURAL REQUIREMENTS FOR EACH SPECIFIC PROJECT. DESIGN PROFESSIONAL TO DESIGN OR CONFIRM ADEQUATE PANEL ATTACHMENT. REFER TO GENERAL NOTES SECTION FOR ADDITIONAL GUIDANCE.

ROOF PANELS ATTACHED	FASTENER WITH BONDED	,✓	LAP
THROUGH TOP OF RIBS	SEALING WASHER TYP.

,�BUTYL TAPE	SCREW OR SEALANT

ROOF INSTALL	C	WALL INSTALL
NU-WAVE CORRUGATED FASTENER INSTALLATION	

'-""
UIL		ING UCT-	NU-WAVE

	
PANEL DETAILS	
		index	NW-01
.J	
REV. 3/13/26

Description

Length(s)

Use

#9 Hex Head Wood Screw (1/4" Drive) with Sealing Washer	1", 1-1/2"
2", 2-1/2"
3"	
Panel to dimensional lumber attachments. Color matched.	
#14 Hex Head Wood Screw (5/16" Drive) with Sealing Washer	1"
1-1/2"	Panel to plywood/OSB attachments (7/16" minimum thickness). Color matched.	
#12 Stitch Screw (1/4" Hex Drive) with Sealing Washer	
3/4"	Exposed trim and panel lap attachments. Visible head size matches Item #1 wood screw. Color matched.	
#14 Lap Self Driller (5/16" Hex Drive) with Sealing Washer	
7/8"	Exposed trim and panel lap attachments. Visible head size matches Item #2 wood screw. Color matched.	

1/8" Diameter Stainless Steel Rivet	1/8" Max Grip Length	
Trim to trim, or trim to panel attachments. Color matched.	
#12 Hex Head Self Drill Screw (1/4" Drive)	1", 1-1/2"
2", 2-1/2"	
Panel to steel deck or steel framing attachment. Color matched.	

#10 Pan Head Screw	
1"	
For non-exposed trim to substrate attachments.	

Notes:
The table above shows the fasteners commonly required for ASC Building Products' panel installations. Refer to the enclosed installation details for further guidance.
Panel attachment screws into plywood/OSB must be long enough to fully penetrate through at least 3/8",

or penetrate into solid lumber by at least one inch.
Exposed fasteners must have sealing washers and should be the same color as the panels and trims they attach.
Screws must be properly driven to ensure proper seal and holding strength. Do not underdrive or overdrive the screws.
Note that rivets are not considered watertight.

Proper Installation of Fasteners with Sealing Washers

Correctly Driven

Under Driven

Over Driven

NU-WAVE

FASTENERS

REV. 3/13/26

index

NW-02

ROOF DETAILS	

	NU-WAVE

		
		index	NW-03	
REV. 3/13/26

r

7"

5-3/4"
3-1/2"

4"

3-1/2"
3/4"	1-1/2"
1/2""'
1/2" l 1"
EAVE (E6)	 SCULPTURED EA VE (E7)

INSIDE CLOSURE (SEALED &
SECURED WITH SEALANT)

1" OVERHANG

EAVE TRIM (E6)

TRIM FASTENER W/SEALING WASHER OR RIVET AT 12" O.C. MAXIMUM

CONTINUOUS BEAD OF NON-SKINNING BUTYL TAPE OR SEALANT

OUTSIDE CLOSURE (SEALED &
SECURED WITH SEALANT) SPECIFIED AIR/WATER BARRIER (X)
SUBSTRATE

(X) -  NOT BY ASC	

'-..	4-,-
UIL ING
UCT-	NU-WAVE

	
EAVE	
		index	NW-04
.J	
REV. 3/13/26

	

	  	

	NU-WAVE

	EAVE W/ GUTTER (PRE-HUNG)	
		index	NW-05	
REV. 3/13/26

	

	  	

	NU-WAVE

	EAVE W/ GUTTER (POST-HUNG)	
		index	NW-06	
REV. 3/13/26

3-1/2"
1/2"

4-3/4"

3/4"
1/2""' GABLE TRIM (G19)

CONTINUOUS BEAD OF NON-SKINNING BUTYL TAPE OR SEALANT
GABLE TRIM (G19) OUTSIDE CLOSURE (SEALED
& SECURED WITH SEALANT)

TRIM FASTENER W/SEALING
WASHER OR RIVET AT---------...I.� 12" o.c. MAXIMUM	7ff,'	I

SPECIFIED AIR/WATER
BARRIER (X) SUBSTRATE

(X) -  NOT BY ASC	

---....
UIL		ING UCT-	NU-WAVE

	
GABLE	
		index	NW-07
.J	
REV. 3/13/26

20-3/4"	20-3/4"
3/4"	3/4"

 VALLEY (V6)

INSIDE CLOSURE (SEALED &	EY (V6)

NOTES:	- A RUBBERIZED COLD-APPLIED MEMBRANE IS
PANEL SETBACK 8" MIN FROM VALLEY CENTERLINE.	RECOMMENDED, EXTENDING A MINIMUM OF 3' -0"	UP PROJECT CONDITIONS (SLOPE, ICE, EXCESSIVE SNOW OR	FROM THE CENTER OF THE VALLEY ON EACH SIDE. RAIN) MAY REQUIRE LARGER SETBACK. CONSULT DESIGN	 - BE ADVISED THAT ROOF VALLEYS INSTALLED IN
PROFESSIONAL AS NEEDED FOR ASSISTANCE.	REGIONS OF WILDFIRE RISK MAY REQUIRE AN ALTERNATE
VALLEY MUST BE THE PROPER WIDTH TO ACCOUNT	CONSTRUCTION TO MEET CODE REQUIREMENTS.
FOR SLOPE, SNOW, ICE AND HEAVY RAIN CONDITIONS.	

"-"
UIL	ING
-	UCT-
\..	NU-WAVE

	
VALLEY	
		index	NW-08
.)	
REV. 3/13/26

	NU-WAVE

	
RIDGE	
		index	NW-09	
REV. 3/13/26

3-1/2"	10"	10"
1/2" HEM	1"
2"	1"	1"	2"
1"
1/2"	1/2"
C-METAL  (C13)	 VENTED RIDGE (RH168)

OUTSIDE CLOSURE

NOTE:
- THIS DETAIL MEETS IWUIC AND CALIFORNIA WUIC FIRE CODE REQUIREMENTS IF: VENT MATERIAL IS NON-COMBUSTIBLE METAL, HAS A CORROSION RESISTANT FINISH (GALVANIZED, OR SIMILAR), AND HAS VENT HOLES BETWEEN 1/16" AND 1/8"
(X) -  NOT BY ASC	IN DIAMETER.	

'-.	.._,
UIL	ING
UCT�	NU-WAVE

	
VENTED RIDGE	
		index	NW-10	
REV. 3/13/26

r

(VARIES)

-	,
(VARIES)	1/2"

./1/2"

PEAK (PF16)

OUTSIDE CLOSURE (SEALED &
s

PEAK TRIM (PF16)

TRIM FASTENER W/SEALING WASHER OR RIVET AT 12" O.C. MAXIMUM

CONTINUOUS BEAD OF NON-SKINNING BUTYL TAPE OR SEALANT

OUTSIDE CLOSURE (SEALED &
SECURED WITH SEALANT) SPECIFIED AIR/WATER BARRIER (X)
SUBSTRATE

(X)  -  NOT BY ASC	

UIL """"'ING
-	ucT~	NU-WAVE

	
PEAK	
		index	NW-11	
REV. 3/13/26

r

5-1/4"

5"
1/2"
SIDEWALL (SW8)

I
I	-r---
1	SPECIFIED AIR/WATER BARRIER (X)
I
I	SUBSTRATE
I	I
I	ii	TRIM FASTENER
I	INSIDE CLOSURE (SEALED &
I	SECURED WITH SEALANT)
+\\\\\\I.	SIDEWALL TRIM (SW8)
I	CONTINUOUS BEAD OF NON-
I	SKINNING BUTYL TAPE OR SEALANT
t n

(X)  -	NOT BY ASC	

'-'
UIL		ING UCT-	NU-WAVE

	
SIDEWALL	
		index	NW-12
.)	
REV. 3/13/26

4-1/2"

6"

..._,
1/2" ENDWALL (EW6)

SPECIFIED AIR/WATER BARRIER (X) SUBSTRATE

ED &
T)
I I
y
OF NON-
TAPE OR SEALANT

E (SEALED &
EALANT)

(X) -  NOT BY ASC	

"'-"
UIL	ING
UCT-
\..	NU-WAVE

	
ENDWALL	
		index	NW-13
.)	
REV. 3/13/26

	  	

	NU-WAVE

	
HI-LO TRANSITION	
		index	NW-14	
REV. 3/13/26

r

INSIDE CLOSURE (SEALED &
SECURED WITH SEALANT)

CONTINUOUS BEAD OF NON-SKINNING BUTYL TAPE OR SEALANT

TRANSITION FLASHING

BLOCKING, AS REQ'D (X)

TRANSITION SUPPORT (X)

OUTSIDE CLOSURE (SEALED & SECURED WITH SEALANT)

(X) -  NOT BY ASC	

'-'
UIL		ING UCT-	NU-WAVE

	
LO-HI TRANSITION	
		index	NW-15
.J	
REV. 3/13/26

	NU-WAVE

	
PANEL LAP	
		index	NW-16	
REV. 3/13/26

RIDGE CAP

RUN UPHILL TRIM UNDER RIDGE CAP

0

0

0	ROOF CURB

0

0

CONTINUOUS BEAD OF NON-SKINNING BUTYL TAPE OR SEALANT ALONG ENTIRE LENGTH OF
PANEL & TRIM LAP	OUTSIDE CLOSURE (SEALED &
SECURED WITH SEALANT)

SEE FOLLOWING PAGE FOR EXPLODED VIEW.	

'-..	�
UIL	ING
-	UCT-	NU-WAVE

	
ROOF CURB	
		index	NW-17
.J	
REV. 3/13/26

   

	NU-WAVE

	
CURB FLASHINGS	
		index	NW-18	
REV. 3/13/26

VERTICAL WALL DETAILS	

	NU-WAVE

		
		index	NW-19	
REV. 3/13/26

r

2-1/8"
1/2" r
1"
1/2"	1-1/2"
1/2""'HEM	3/4"
 DRIP EDGE (81)	 (OPTIONAL) WC215

SUBSTRATE

SPECIFIED AIR/WATER BARRIER (X)
�	BUTYL FLASHING TAPE
J.	(MAS.025BF)
I
PANEL FASTENER

INSIDE CLOSURE (SEALED & SECURED WITH SEALANT)
OPTIONAL EDGE FLASHING (WC215)

FLASHING FASTENER

DRIP FLASHING (81)

(X) -  NOT BY ASC	

'-""
UIL	ING
-	UCT-	NU-WAVE

	
BASE	
		index	NW-20
.)	
REV. 3/13/26

		

I	I	

112 .. r		
		�	1-1/2"		
			3/4"		
			 (OPTIONAL) WC215		

SUBSTRATE		
			SPECIFIED AIR/WATER BARRIER (X)		
			BUTYL FLASHING TAPE (MAS.025BF)		
			PANEL FASTENER		
			INSIDE CLOSURE (SEALED &		
			SECURED WITH SEALANT)		
			OPTIONAL EDGE FLASHING		
			(WC215)		

FLASHING FASTENER		
		
 L_		t1/4' GAP		
			t		
			SILL FLASHING (V)		
					
			ALTERNA TE WALL MATERIALS		

(X)  -	

NOT BY ASC				
(V)  -	DIMENSIONS	VARY BASED ON PROJECT	CONDITIONS		

"-'
UIL		ING UCT-
'-	NU-WAVE

	
SILL	
		index	NW-21	

_	

r

)
REV. 3/13/26

3-1/2"	3-1/2"			
			1/2" HEM	1"	1/2" HEM	1''			
			/			
			1"	1"			
			C-METAL  (C13)	 JAMB TRIM (J13)			

.d					
	<1					
	<:3					
	.d					
	
<1		SPECIFIED AIR/WATER	BARRIER (X)		
	
.d	<1		SUBSTRATE			
	<:3					
	
ti.
"
<1	.d	

�	
�		 -	_/	'			
	
<1

<ZI	.d	
				
	<:3					
	<1					
	.d					
	<1					
	<:3					
	.d					
			CONTINUOUS BEAD OF NON-			
			SKINNING BUTYL TAPE OR SEALANT			
			TRIM FASTENER W/SEALING WASHER			
			OR RIVET AT 12" O.C. MAXIMUM			
			C-METAL (C13)			
			SEALANT/  BACKER  ROD			

(X)  -	

NOT BY ASC					

"'-"
UIL	ING
UCT-
\..	NU-WAVE

	
END WALL	
		index	NW-22	
.J	
REV. 3/13/26

r

1/2" HEM r

3-1/2"

SYMMETRIC�

OUTSIDE CORNER (OC2)

r;	ill

SUBSTRATE SPECIFIED AIR/WATER BARRIER (X)

CONTINUOUS BEAD OF NON-SKINNING BUTYL TAPE OR SEALANT

PANEL FASTENER W/SEALING WASHER OR RIVET AT 12"  O.C. MAXIMUM

OUTSIDE CORNER TRIM (OC2)

(X) -  NOT BY ASC	

"-""
UIL		ING UCT-
\..	NU-WAVE

	
OUTSIDE CORNER	
		index	NW-23
.)	
REV. 3/13/26

	SYMMETRICAL

3-1/4"
1/2" HEM l

r.
INSIDE CORNER (IC2)

=	=		j

SUBSTRATE

SPECIFIED AIR/WATER BARRIER (X) INSIDE CORNER TRIM (IC2)

ENER W/SEALING WASHER 12" O.C. MAXIMUM

BEAD OF NON-SKINNING BUTYL TAPE OR SEALANT

(X)  -  NOT BY ASC	

'--"
UIL	ING
UCT-
'-	NU-WAVE

	
INSIDE CORNER	
		index	NW-24
..	

)
REV. 3/13/26

r

(V)	1/2"
1/2"
135"
2-1/8"
 COVER TRIM
1"
1/2"
�
1/2" HEM
DRIP EDGE (81)
I
I
I	I
�

SUBSTRATE SPECIFIED AIR/WATER BARRIER (X)

BUTYL FLASHING TAPE
(MAS.025BF)

INSIDE CLOSURE (SEALED & SECURED WITH S

1/4'

OUTSIDE CLOSURE (SEALED &
DRIP EDGE (81)	SECURED WITH SEALANT)
CONTINUOUS BEAD OF NON-
COVER TRIM (V)	SKINNING BUTYL TAPE OR SEALANT
TRIM FASTENER W/SEALING WASHER OR RIVET AT 12" O.C. MAXIMUM
(X) -  NOT BY ASC
(V) - DIMENSIONS VARY BASED ON PROJECT CONDITIONS	

'-..	�
UIL		ING UCT-	NU-WAVE

	
SOFFIT (FRONT)	
		index	NW-25
.J	
REV. 3/13/26

	SYMMETRICAL		

ij

J					
3-1/4"							
1/2" HEM l							
INSIDE CORNER (IC2)							
				I I I I			
				
V:			

I	I I I I			
OUTSIDE CLOSURE (SEALED &
SECURED WITH SEALANT)							
	�						
INSIDE CORNER TRIM (IC2)							
TRIM FASTENER W/SEALING WASHER OR RIVET AT 12" O.C. MAXIMUM							
CONTINUOUS BEAD OF NON-SKINNING BUTYL TAPE OR SEALANT							

SPECIFIED AIR/WATER BARRIER (X)							
SUBSTRATE							

(X) -  NOT BY ASC							

UIL""'ING
UCT-
'-	NU-WAVE

	
SOFFIT (BACK)	
		index	NW-26	

.)	
REV. 3/13/26

r

PARAPET FLASHING (V) BLOCKING (AS REQUIRED)

TRIM FASTENER W/SEALING WASHER OR RIVET AT 12" O.C. MAXIMUM

CONTINUOUS BEAD OF NON-SKINNING BUTYL TAPE OR SEALANT
OUTSIDE CLOSURE (SEALED &
SECURED WITH SEALANT)

SPECIFIED AIR/WATER BARRIER (X)

SUBSTRATE

(X) -  NOT BY ASC
(V) - DIMENSIONS VARY BASED ON PROJECT CONDITIONS	

1/4:12 MIN. SLOPE	

		

�
UIL	ING
-	ucT~	NU-WAVE

	
PARAPET	
		index	NW-27	
.J	
REV. 3/13/26

		

	  	

	NU-WAVE

	DOOR / WINDOW (HEAD)	
		index	NW-28	
REV. 3/13/26

	

	

	NU-WAVE

	OPENING, HEAD (NAIL FIN)	
		index	NW-29	
REV. 3/13/26

	  	

	NU-WAVE

	DOOR / WINDOW (JAMB)	
		index	NW-30	
REV. 3/13/26

  

	NU-WAVE

	OPENING, JAMB (NAIL FIN)	
		index	NW-31	
REV. 3/13/26

	

 

	  	

	NU-WAVE

	DOOR / WINDOW (SILL)	
		index	NW-32	
REV. 3/13/26

  

	NU-WAVE

	OPENING, SILL (NAIL FIN)	
		index	NW-33	
REV. 3/13/26

 	

   

	

	NU-WAVE

	
PENETRATION (3D)	
		index	NW-34	
REV. 3/13/26

r

I
�	I	I
I
I	I
-====J:	I
,	I	I	I
I
I	I
I	I
_J	I	I
VERTICAL DRIP TRIM (X)	---t-L	+-
W/FASTENER & BUTYL TAPE	I	I
I	I	I
SEAL PENETRATION PERIMETER	I	I
WITH POLYURETHANE SEALANT	I	I
;	I	I
I	I
I	I
I
WALL PENETRATION	Jr- :	I
I	I
SPECIFIED	I	I
AIR/WATER BARRIER (X)	+	--------,--
SUBSTRATE	�	�
�	I
I

�

PENETRATION COVER (X)

BOTTOM COVER TRIM (X)

(X) -  NOT BY ASC	

'-'
UIL		ING UCT-	NU-WAVE

	
PENETRATION (2D)	
		index	NW-35
.J	
REV. 3/13/26

	

	NU-WAVE

	PENETRATION (3D) EXAMPLES	
		index	NW-36	
REV. 3/13/26

HORIZONTAL WALL DETAILS	

	NU-WAVE

		
		index	NW-37	
REV. 3/13/26

r

2-1/8"
1"
"'1/2"
3/8"  HEM
 DRIP EDGE (B1)

PANEL FASTENER SUBSTRATE
SPECIFIED AIR/WATER BARRIER (X)

BUTYL FLASHING TAPE (MAS.025BF)

t 1/4' GAP
<1	4	<1 <I	t
4	�
<1
<I	<1
<I	<I	"'
<1	<I
<1	<I	<I
<1
DRIP FLASHING (B1)
A	<1

HORIZONTAL NU-WAVE PANELS ARE INSTALLED FROM GROUND TO EAVE.

(X)  -  NOT BY ASC	

'--"
UIL		ING UCT-
\..	NU-WAVE

	
BASE	
		index	NW-38
.J	
REV. 3/13/26

r

SUBSTRATE

SPECIFIED AIR/WATER BARRIER (X) BUTYL FLASHING TAPE (MAS.025BF)
PANEL FASTENER

		�  1/4' GAP
t

SILL FLASHING (V) ALTERNATE WALL MATERIALS

(X) -  NOT BY ASC
(V) - DIMENSIONS VARY BASED ON PROJECT CONDITIONS	

'-'
UIL		ING UCT-
\..	NU-WAVE

	
SILL	
		index	NW-39
.)	
REV. 3/13/26

r
l

EAVE FLASHING (V)

TRIM FASTENER W/SEALING WASHER OR RIVET AT 12" O.C. MAXIMUM

CONTINUOUS BEAD OF NON-SKINNING BUTYL TAPE OR SEALANT
I I I I I
I  I
�
I

SPECIFIED AIR/WATER BARRIER (X)

SUBSTRATE
...._
PANEL FASTENER

(X) -  NOT BY ASC
(V) - DIMENSIONS VARY BASED ON PROJECT CONDITIONS	

""--"
UIL		ING UCT-
\..	NU-WAVE

	
EAVE / FASCIA	
		index	NW-40
.)	
REV. 3/13/26

3-1/2"	3-1/2"
1/2" HEM	1"	1/2"	1"
1"	1"
C-METAL  (C13)	 JAMB TRIM (J13)

'1

q
4
'1

q	SPECIFIED AIR/WATER BARRIER (X)
'1	q	SUBSTRATE
4

11
," �l!- -			'
q	'1
�
q

<:II	'1
4
q

'1

q
4
'1
OUTSIDE CLOSURE (SEALED &
SECURED WITH SEALANT)
CONTINUOUS BEAD OF NON-SKINNING BUTYL TAPE OR SEALANT

TRIM FASTENER W/SEALING WASHER OR RIVET AT 12" O.C. MAXIMUM
C-METAL (C13)

SEALANT/ BACKER ROD

(X)  -  NOT BY ASC	

�
UIL	ING
-	UCT-
\..	NU-WAVE

	
END WALL	
		index	NW-41
.J	
REV. 3/13/26

r

(X) -	

1/2" HEM r

3-1/2"

SYMMETRIC�

OUTSIDE CORNER (OC2)

SUBSTRATE SPECIFIED AIR/WATER BARRIER (X)

_.1_	'

OUTSIDE CLOSURE (SEALED &
SECURED WITH SEALANT)

CONTINUOUS BEAD OF NON-SKINNING BUTYL TAPE OR SEALANT

TRIM FASTENER W/SEALING WASHER OR RIVET AT 12" O.C. MAXIMUM

OUTSIDE CORNER TRIM (OC2)

NOT BY ASC	

r,	

ill	

"	I

			

'-""
UIL	ING
-	UCT-	NU-WAVE

	
OUTSIDE CORNER	
		index		NW-42	
.J	
REV. 3/13/26

r

r;	

=

◄
I  	

�	SYMMETRICAL		
				
3-1/2"		
				1/2"  HEM		
				INSIDE CORNER (IC2)		

=				

	 		

SUBSTRATE

SPECIFIED AIR/WATER BARRIER (X)		
				INSIDE CORNER TRIM (IC2)		

 FASTENER W/SEALING WASHER		
				 VET AT 12" O.C. MAXIMUM		
				 NUOUS BEAD OF NON-		
				ING BUTYL TAPE OR SEALANT		
				  DE CLOSURE (SEALED &		
				SECURED WITH SEALANT)		

(X)  -	

NOT BY ASC					

"--	'-"
UIL	ING
UCT-	NU-WAVE

	
INSIDE CORNER	
		index	NW-43	
.J	
REV. 3/13/26

(V)	1/2"
1/2"
135"
2-1 /8"
COVER TRIM
1"
1/2"
�
3/8" HEM DRIP EDGE (B1)

SUBSTRATE SPECIFIED AIR/WATER BARRIER (X)

BUTYL FLASHING TAPE
(MAS.025BF)

t
1/4'  GAP
t
OUTSIDE CLOSURE (SEALED &
DRIP EDGE (B1)	SECURED WITH SEALANT)
CONTINUOUS BEAD OF NON-SKINNING BUTYL TAPE OR SEALANT
TRIM FASTENER W/SEALING WASHER OR RIVET AT 12" O.C. MAXIMUM
COVER TRIM (V)

(X) -  NOT BY ASC
(V) - DIMENSIONS VARY BASED ON PROJECT CONDITIONS	

.-...,
UIL		ING UCT-	NU-WAVE

	
SOFFIT (FRONT)	
		index	NW-44
.J	
REV. 3/13/26

r

	SYMMETRICAL 3-1/4"
1/2" HEM l

INSIDE CORNER (IC2)

I I I I I
"I
I I I
I	I
I
OUTSIDE CLOSURE (SEALED &	.I\\\UI>
SECURED WITH SEALANT)

INSIDE CORNER TRIM (IC2)

TRIM FASTENER W/SEALING WASHER OR RIVET AT 12" O.C. MAXIMUM

CONTINUOUS BEAD OF NON-SKINNING BUTYL TAPE OR SEALANT

SPECIFIED AIR/WATER BARRIER (X)

SUBSTRATE

(X) -  NOT BY ASC	

"--	4-,,
UIL ING
-	ucT~	NU-WAVE

	
SOFFIT (BACK)	
		index	NW-45
.J	
REV. 3/13/26

r

1/4:12 MIN. SLOPE

PARAPET FLASHING (V) BLOCKING (AS REQUIRED)

TRIM FASTENER W/SEALING WASHER OR RIVET AT 12" O.C. MAXIMUM

CONTINUOUS BEAD OF NON-SKINNING BUTYL TAPE OR SEALANT

SPECIFIED AIR/WATER BARRIER (X)

SUBSTRATE

(X)  -  NOT BY ASC
(V)  -  DIMENSIONS VARY BASED ON PROJECT CONDITIONS	

"-..	�
UIL		ING UCT-	NU-WAVE

	
PARAPET	
		index	NW-46
.J	
REV. 3/13/26

		

	  	

	NU-WAVE

	DOOR / WINDOW (HEAD)	
		index	NW-47	
REV. 3/13/26

	 	

	NU-WAVE

	OPENING, HEAD (NAIL FIN)	
		index	NW-48	
REV. 3/13/26

	  	

	NU-WAVE

	DOOR / WINDOW (JAMB)	
		index	NW-49	
REV. 3/13/26

	      	

	NU-WAVE

	OPENING, JAMB (NAIL FIN)	
		index	NW-50	
REV. 3/13/26

 

	  	

	NU-WAVE

	DOOR / WINDOW (SILL)	
		index	NW-51	
REV. 3/13/26

	  	

	NU-WAVE

	OPENING, SILL (NAIL FIN)	
		index	NW-52	
REV. 3/13/26

   

 

	  	

	NU-WAVE

	
WALL PENETRATION (3D)	
		index	NW-53	
REV. 3/13/26

TRIM FASTENER W/SEALING
WASHER OR RIVET
I
I I I I I
SPECIFIED	I
AIR/WATER BARRIER (X)	I
I
SUBSTRATE	_j	
I
I I
SEAL PENETRATION PERIMETER	I
WITH POLYURETHANE SEALANT	I
I
�
WALL PENETRATION	I
I
PENETRATION COVER (X)	I
I
OPTIONAL FIELD FABRICATED	I
CLOSURE COVER TRIM (X)	I
-i-
i I I I I I

(X) -  NOT BY ASC	

4-,
UIL		ING UCT-
'-	NU-WAVE

	
PENETRATION (2D)	
		index	NW-54
.J	
REV. 3/13/26

	

	

	NU-WAVE

	PENETRATION (3D) EXAMPLES	
		index	NW-55	
REV. 3/13/26

MANUFACTURING FACILITY:
California
2110 Enterprise Boulevard West Sacramento, CA 95691

Oregon
4063 Salem Industrial Ave NE Salem, OR 97301

Washington 4111 East Ferry Ave. Spokane, WA 99202

CUSTOMER SERVICE:
Oregon
800-272-7023

Washington
509-536-4097

Visit us at:
www.ascbp.com

®

©2026 ASC Profiles LLC. All rights reserved.