SKYLINE ROOFING®	®

Skyline Roofing®
Skyline Roofing is a standing seam metal panel with a concealed fastener design. With clean lines and lasting performance, Skyline Roofing panels have long been a top choice for residential roofing.

STANDING BY OUR PRODUCTS AND WARRANTIES FOR OVER 50 YEARS

FEATURES AND BENEFITS
12" and 16" coverage roof panel.
Minimum recommended slope 3:12.
Available in 26ga Dura Tech™ xl colors and the 16" panel is also available in ZINCALUME® Plus and Natural Rust.
Limited Lifetime Warranty for residential applications.
Custom manufactured panel lengths: 4'-0" to up to 50'-0".
Subtle striations available - Additional lead times may apply.
Snap-together panel, no field seaming required.
Testing: ASTM E1592 (wind uplift) All testing performed by accredited third-party.
Roof assemblies Class A Fire Rated when installed on non-combustible deck or framing per IBC, IRC or when installed in accordance to UL listings (UL790).
Class 4 Impact (Hail) Resistance rated per UL 2218.
Panel evaluated by accredited third party. All structural performance data is contained within Building Code Approval Report: IAPMO-UES #ER-0309.

 1"

1"

Skyline Roofing®

 12" and 16" net coverage 

Skyline Roofing® (Striated Option)

(Additional Lead Times May Apply)

 12" and 16" net coverage 

Customer Service Centers
Salem, OR: 503-390-7174 or 800-272-7023 I Spokane, WA: 509-536-4097 or 800-776-8771

www.ascbp.com

Keeps the heat out and the color brilliant.
Superior color retention • Chalk and fade resistant • Energy saving colors.

Standard Offer

Forest Green SRI: 36 • LRV: 8

Slate Gray SRI: 32 • LRV: 13

Rustic Red SRI: 43 • LRV: 13

Classic Brown SRI: 29 • LRV: 7

ZINCALUME® Plus SRI: 64 • LRV: 67

Denali Green SRI: 29 • LRV: 11

Old Town Gray SRI: 43 • LRV: 27

Patina Steel SRI: 38 • LRV: 17

Chestnut Brown SRI: 36 • LRV: 12

Copper Penny* SRI: 53 • LRV: 28

Everglade SRI: 35 • LRV: 19

Zinc Gray SRI: 43 • LRV: 22

Matte Black SRI: N/A • LRV: 5

Light Stone SRI: 70 • LRV: 53

Natural Rust* SRI: 32 • LRV: 10

Tahoe Blue SRI: 33 • LRV: 14

Weathered Copper SRI: 32 • LRV: 11

Winter White SRI: 88 • LRV: 74

Taupe

SRI: 53 • LRV: 28

ASC Building Products is Proudly Distributed by:

All information stated in the product sheet is correct at time of printing and subject to change without notice, check our website for the latest version.
2025 ASC Profiles LLC. All rights reserved. ZINCALUME® is a registered trademark of BlueScope Steel Ltd. 0825 web (PS131)

www.ascbp.com

REPRESENTATION OF COLORS MAY VARY DUE TO PRINTING LIMITATIONS.
Sample color chips are available upon request. Consult your ASC Building Products representative for more information.

SKYLINE ROOFING®

®

* Please note these colors are batch sensitive (may have color variation) and are directional in nature. Different batches are not to be mixed on projects. We recommend that you request a sample of current stocked material to review actual color before ordering to ensure color accuracy. We are not responsible for color variations. Color inventory may vary by manufacturing facility and gauge. Please inquire with customer service for availability.