®

IRONOX CORRUGATED

Please Note: Finish varies at time of order

IronOx Corrugated
IronOx Corrugated panel is ideal for creative
builders looking to design with the aesthetic beauty of rusted corrugated steel. Its historic corrugated
form preserves the old-fashioned design of steel panels that have graced the countryside for
decades.
FEATURES AND BENEFITS
Heavy 22 gauge steel with 36" out-to-out width.

Unpainted and untreated steel allows the surface to rust and form a natural iron oxide finish.
Matching flat sheet offered in 46" width.
Fastener options; plated/painted fasteners in Terra-Cotta color.
RECOMMENDATIONS AND CAUTIONS
Performs best in environments with low humidity, not recommended near salt spray and frequent rain locations

7⁄8"

22⁄3"

36" Out-to-Out

32" Net Coverage* (Roof only) 342⁄3" Net Coverage (Wall only)

* IronOx Corrugated does not meet the minimum requirements for a metal roof covering per the IBC® and IRC®. Check the building code requirements for your
project before ordering or installing.
IronOx Corrugated meets ASTM A-1008 Cold Rolled annealed, does not meet ASTM A606-96 Type 4.

as it will shorten the life of the panel.
IronOx Corrugated will continue to rust for life of the panel. Acid washing will degrade the steel performance.
Rust runoff will likely stain the surrounding surfaces.

ASC Building Products does not provide any warranties, expressed or
implied, on 22 gauge black steel (cold-rolled bare steel) referred to as IronOx Corrugated. This product is intended to naturally weather and rust. ALL WARRANTIES, EXPRESSED OR IMPLIED, ARE DISCLAIMED AND EXCLUDED, INCLUDING WITHOUT LIMITATION ANY IMPLIED WARRANTY OF MERCHANTABILITY OR FITNESS FOR A PARTICULAR PURPOSE OR USE.

Customer Service Centers

IBC® and IRC® are registered trademarks of International Code Council, Inc.

Photo credit: Nuvue Interactive

Salem, OR: 503-390-7174 or 800-272-7023 I Spokane, WA: 509-536-4097 or 800-776-8771
©2016-2024 ASC Profiles LLC. All rights reserved. 0224  WEB  (PS160)

www.ascbp.com