PBR Panel

PBR Panel

The PBR Panel is an ideal solution for pre- engineered metal, post-frame, and agricultural buildings. This panel is recommended for
light commercial and industrial projects as well as consumer-based Do-It-Yourself (DIY) applications.
FEATURES AND BENEFITS
36" net panel coverage can be installed over solid

11⁄4"

 	

PANEL OVERVIEW

12"

36" Net Coverage

substrates or spaced support members.
Purlin-bearing leg speeds installation and improves the quality of panel side laps providing a consistent weather-resistant joint.
Provides traditional metal roof or wall appearance with 11⁄4" high trapezoidal major ribs at 12" on center with minor ribs between each major rib.
Trim packages available in the same gauge and color as the roof and wall panel.
PBR Panel can be installed on pitches as low as 1:12 with field applied mastic.
Matching polycarbonate panels available.

Available in Dura Tech™ nt colors and ZINCALUME® Plus.

ZINCALUME coated substrate, per ASTM A792, is standard and backed by a limited corrosion warranty  on painted or unpainted panels. It is not recommended for use in structures where exposure to animals and/or animal waste will occur.
Building Code Approval Report: #ER-0550

Customer Service Centers
Salem, OR: 503-390-7174 or 800-272-7023 I Spokane, WA: 509-536-4097 or 800-776-8771

www.ascbp.com

ZINCALUME® Plus

Desert Beige

Weathered Copper

Winter White
(G90 only)

Old Town Gray

Denali Green

Surf White

Chestnut Brown

Light  Stone

Rustic Red
(Available from Sacramento only)

The Dura Tech™ nt system combines the protection of ZINCALUME® with a highly durable COOL Resin technology to reduce the demand for energy and provide excellent color retention.

PAINT FINISH NOTES
All PBR Panels are available in standard, 26 gauge, Dura Tech nt colors, as well as ZINCALUME Plus. Inquire with a sales representative for lead times and more information.

AVAILABILITY
PBR Panel is available out of Sacramento, CA and Spokane, WA. Additional lead times apply on products supplied from a non-local facility.
FLASHINGS & TRIM
All trims and flashings are offered in standard, 26 gauge, Dura Tech nt colors, as well as ZINCALUME Plus. Inquire with a sales representative for more information.

OIL CANNING
All flat metal surfaces can display waviness commonly referred to as “oil canning”. “Oil canning” is an inherent characteristic of steel products, not a defect, and therefore is not a cause for panel rejection.

REPRESENTATION OF COLORS MAY VARY DUE TO
PRINTING LIMITATIONS. Sample color chips are available upon request. Consult your ASC Building Products representative for more information.

LOAD TABLE

Gauge	
Span	
Cond.	Positive (Inward) Uniform Load Capacity (lbs/ft2) / Span (ft.-in.)	
			2'-0"	2′-6"	3'-0"	3'-6"	4'-0"	5'-0"	6'-0"	7'-0"	8'-0"	

26	Single Span	ASD, W/Ω	240	153	107	78	60	38	27	20	15	
		L/180	-	-	-	-	-	32	19	12	8	
	Double Span	ASD, W/Ω	252	166	117	86	66	43	29	21	17	
		L/180	-	-	-	-	-	-	-	-	-	
	Triple Span	ASD, W/Ω	307	203	144	107	82	53	38	27	21	
		L/180	-	-	-	-	-	-	35	22	15	
NOTES:
Top values based on allowable stress (ASD). Bottom values based on a deflection limit of L/180. “-” denotes that the allowable load is limited by the panel stress vs. deflection limit.
Steel conforms to ASTM A653 (Galvanized) or ASTM A792 (ZINCALUME) structural steel. Tabulated values are for positive (inward) uniform loading only.

ASC Building Products' Roofing and Siding is the Building Choice You Can Make with Confidence.

Values are based on the American Iron and Steel Institute “Cold Formed Steel Design Manual” (AISI S100-12). Refer to ascbp.com for more complete PBR Panel performance data.

Five lasting advantages of steel . . .
Outstanding Value Reduced Energy Costs Long-Term Protection Non-Combustible
Low Maintenance

Properties	

Gauge	Base Steel
Thickness (in)	Yield (ksi)	Tensile (ksi)	Wt. (lbs/ft2)	I+
(in4/ft)	S+
(in3/ft)	I-
(in4/ft)	S-
(in3/ft)	
26	0.0173	80	82	0.85	0.0463	0.0400	0.0394	0.0457	
NOTES: The moments of inertia, I+ and I-, presented for determining deflection are: (2IEffective + IGross)/3

Inward Loads	
Single Span	w, distributed load	
				L, span			

Double Span	w
 	
L	L	
	
Triple Span	w

L	L	L	

ASC Building Products is Proudly Distributed by:

PBR Panel

All information stated in the product sheet is correct at time of printing and subject to change without notice, check our website for the latest version.
©2013-2019 ASC Profiles LLC. All rights reserved. ZINCALUME® is a registered trademark of BlueScope Steel Ltd. 0819 150 (PS178)

www.ascbp.com