DESIGN SPAN® hp	®

Design Span hp

EXCELLENCE IN STANDING SEAM STEEL ROOFING

When you're looking for protection, beauty, and value in a roof, a distinctive standing seam panel offers the best solution. Design Span hp is a concealed fastener system which offers performance and beauty.

Subtle striations between ribs reduce the appearance of oil-canning.

1¾"

FEATURES AND BENEFITS
24 and 22ga available in our Dura Tech™ 5000
and Dura Tech™ mx colors.

12", 16", & 17" Net Coverage

Limited Lifetime Warranty for residential applications.
Recommended minimum slope of 2:12. Inquire for slopes below 2:12.
Factory notching available for turn under at the eave (some limitations apply). Notch provides a clean detail and reduction in labor.
A snap-on panel requiring no field seaming, and comes standard with factory applied sealant in the female leg for reduced field labor and ease of installation.
Tested for air infiltration per ASTM E1680, water infiltration per ASTM E1646, and wind uplift per ASTM E1592.
Product is UL Class A Fire Rated when installed in accordance with UL requirements.

Panel evaluated by accredited third party. All structural performance

(18" available – additional charges and lead times apply)

Optional 11⁄8" factory end
notch to help reduce field labor and make installation easier.

Customer Service Centers
Salem, OR: 503-390-7174 or 800-272-7023 I Spokane, WA: 509-536-4097 or 800-776-8771

www.ascbp.com

data is contained within an IBC/IRC code compliance report.	Factory notch allows panel to be field turned down with clean, uniform detail.

PROJECT DESIGNED BY COATES DESIGN ARCHITECTS

®
5000
These Energy Saving Cool Colors
keep the Heat Out and the Color Brilliant.

ZINCALUME® Plus SRI: 64 • LRV: 67

Cool Regal White SRI: 88 • LRV: 75

Cool Parchment SRI: 58 • LRV: 40

Cool Sierra Tan SRI: 55 • LRV: 34

   

Cool Pebble SRI: 48 • LRV: 27

Cool Walnut SRI: 38 • LRV: 18

Cool Weathered Copper SRI: 34 • LRV: 11

Cool Dark Bronze SRI: 32 • LRV: 8

Cool Terra-Cotta SRI: 41 • LRV: 15

Cool Colonial Red SRI: 35 • LRV: 9

Cool Old Town Gray SRI: 43 • LRV: 27

Cool Zinc Gray SRI: 39 • LRV: 20

Cool Slate Gray SRI: 33 • LRV: 12

Cool Midnight Bronze SRI: 27 • LRV: 7

Cool Matte Black SRI: 29 • LRV: 5

Cool Tahoe Blue SRI: 33 • LRV: 14

   

Cool Regal Blue SRI: 29 • LRV: 10

Cool Sage Green SRI: 41 • LRV: 21

Cool Leaf Green SRI: 30 • LRV: 11

Cool Forest Green SRI: 29 • LRV: 9

Vintage®* SRI: 22 • LRV: 20

Vintage® coated metal is available in 24ga only. Vintage is an innovative coating processed over galvanized G90 metallic- coated steel substrate producing a beautiful, durable, aged- metallic finish.

®

Energy Savings in long lasting Cool Metallic Colors

Cool Metallic Silver* SRI: 65 • LRV: 50

Cool Silversmith* SRI: 58 • LRV: 54
Note*

Cool ZACtique® II* SRI: 39 • LRV: 22

Cool Metallic Champagne* SRI: 54 • LRV: 33

Cool Metallic Copper* SRI: 53 • LRV: 29

Oil Canning
All flat metal surfaces can display waviness commonly referred to as “oil canning.”

“Oil canning” is an inherent characteristic of steel products, not a defect, and therefore is not a cause for panel rejection.

Metallic colors are subject to a price upcharge. Metallic coatings are batch sensitive and directional in nature. Minor differences in both color and appearance are normal and
to be expected with metallic coatings, as it is virtually impossible to match one metallic coating to another. Due to the coil application process, striations and longitudinal patterning may also show on these products. To minimize the possible visual effects
of the normal minor differences in paint and its application, an entire job should be painted at one time. Additionally, fabricated panels, flat sheets, and flashings should be orientated in the same direction for installation.

ASC Building Products is Proudly Distributed by:

REPRESENTATION OF COLORS MAY VARY DUE TO PRINTING LIMITATIONS.
Sample color chips are available upon request. Consult your ASC Building Products representative for more information.

DESIGN SPAN® hp

®

SRI=Solar Reflective Index. SRI values in accordance with ASTM E1980 and are based on independent testing. Cool Roof Rating Council (CRRC) performance values (for CA Title 24) are based on color families and will differ from those listed above. Please visit www.ascbp.com for additional information.
All information stated in the product sheet is correct at time of printing and subject to change without notice, check our website for the latest version.
©2007-2024 ASC Profiles LLC. All rights reserved. ZINCALUME® is a registeredtrademark of BlueScope Steel Ltd. 0224  web  (PS225)

www.ascbp.com