®

SKYLINE ROOFING® hp

Customer Service Centers
Salem, OR: 503-390-7174 or 800-272-7023 I Spokane, WA: 509-536-4097 or 800-776-8771

www.ascbp.com

Skyline Roofing hp
Skyline Roofing hp is a 24 gauge high
performance panel available in durable premium colors. This concealed fastened, standing seam
panel is ideal for residential and light commercial roof applications.
FEATURES AND BENEFITS
Available in our Dura Tech™ 5000 and Dura Tech™ mx colors, which are energy efficient, cool colors, formulated to help reduce the demand for energy.
Limited Lifetime Warranty for residential applications.
ASTM E1592 tested for wind uplift performance.
Skyline Roofing hp panel assemblies are Class
A Fire Rated when installed on non-combustible
deck or framing per IBC, IRC, or UL790 when installed in accordance to UL listings.

Panel evaluated by accredited third party.
All structural performance data is contained within an IBC/IRC 2015 code compliance report.

STANDING BY OUR PRODUCTS AND WARRANTIES FOR OVER 50 YEARS

 1"

Skyline Roofing hp

	16" Net Coverage	

(Available in Salem, OR. Additional Lead Times May Apply)

Skyline Roofing hp Striated Option (not pictured)

 1"

16" Net Coverage

5000
These Energy Saving Cool Colors
keep the Heat Out and the Color Brilliant.
Standard Offer

Energy Savings in long lasting Cool Metallic Colors.
Special Order

Cool Weathered Copper
SRI: 34

Cool Dark Bronze
SRI: 32

Cool Old Town Gray
SRI: 43

Cool Zinc Gray
SRI: 39

Cool Metallic Copper†
SRI: 53

Cool Metallic Champagne†
SRI: 54

Cool Metallic Silver†
SRI: 65

Cool Slate Gray
SRI: 33

Cool Matte Black
SRI: 29

Cool Forest Green
SRI: 29

† Metallic colors are subject to a price up charge. Metallic coatings are batch sensitive and directional in nature. Minor differences in both color and appearance are normal and to be expected with metallic coatings, as it is virtually impossible to match one metallic coating to another. Due to the coil application process, striations and longitudinal patterning may also show on these products. To minimize the possible visual effects of the normal minor differences in paint and its application, an entire job should be painted at one time. Additionally, fabricated panels, flat sheets, and flashings should be orientated in the same direction for installation.

Special Order (Minimum order required)

REPRESENTATION OF COLORS MAY VARY DUE TO PRINTING LIMITATIONS.
Sample color chips are available upon request. Consult your ASC Building Products representative for more information.

METAL STEEL ROOFING

EXCELLENCE IN

ASC Building Products is Proudly Distributed by:

All information stated in the product sheet is correct at time of printing and subject to change without notice, check our website for the latest version.
©2024 ASC Profiles LLC. All rights reserved. ZINCALUME® is a registered trademark of BlueScope Limited. 0224 PS133 web

www.ascbp.com

SKYLINE ROOFING® hp

®

Cool Regal White
SRI: 88

Cool Leaf Green
SRI: 30

Cool Sierra Tan
SRI: 55

ZINCALUME® Plus
SRI: 64

Cool Terra- Cotta
SRI: 41

Cool Regal Blue
SRI: 29

Oil Canning
All flat metal surfaces can display waviness commonly referred to as
“oil canning.” “Oil canning” is an inherent characteristic of steel products, not a defect, and therefore is not a cause for panel rejection.