5-1/2"	

2"	
6"		

Design Span hp 	Skyline Roofing

AL41 Angle Cleat	B41 Drip Flashing	B16 Base Trim	C16 C Trim	

2-3/8"

5/8"	

2"	

3"
1-1/8"
1/2"	
3"
1-1/8"

1"	

CF41 Counter Flashing	G41 Gable	E16 Narrow Eave	E17 Wide Eave	

3-1/2"

1"
1"	1-1/2"
1-1/4"
1/2"
5-7/8"

3/4"	
2"

1-1/8"
Pitch Required	1/2"	4"

3"
5/8"
Pitch Required	

L41 Closure	OL41 Offset Cleat	E18 Snow Eave	E19 Notched Eave	

1-3/4"
2-1/4"	

1-1/2"

5/16"	13/16"	5-1/8"

1-1/4"
1-3/4"
Pitch Required	1/2"	3-1/4"

1-1/4"
Varies
No customs	5/8"
Pitch Required	available	

R41 Ridge	R42 Vented Ridge	E21 Nosed Eave	E22 Nosed Eave	

8-1/2"

Pitch Required	

9"
1-1/2"  3"

Pitch Required	3-3/4"

1-1/4"
1-1/2"
5/8"
Pitch Required	
3-3/4"

1" 1-1/4"
5/8"
Pitch Required	

SF41 Support Flashing	TR41 Transition (High-Low)	EW16 Endwall	EW17 Vented Endwall	
1"

1-3/4"

5-1/4"	

7"	16-1/2"

Pitch Required	

4"

5"
Pitch Required	

4"
6-3/4"
1-1/8"  1-7/8"
Pitch Required	

TR43 Transition (Low-High)	V41 Valley	G5 Adjustable Gable	G16 Narrow Gable	

16-1/2"

7"

Pitch Required	

1/2"
1"
19-1/2"
Pitch Required	6"

4"

1/2"	1/2"
1"	1"

3"

1/2"	

ZL41 “Z” Clip	Z41 “Z” Closure	G17 Standard Gable	G18 Chalet Gable	

2 1/8"
1-3/4"

2” Length	2 1/8"	
2-1/8"

1-3/4"

2-1/8"	2-1/4"
1-1/8"	3/4"
3/8"
4"

1/2"	3/4"
1-5/8"
3-7/8"	6"

5/8"	

Skyline Roofing® 	Nu-Wave® Corrugated  	PBR Panel
PF16 Peak Flashing	PF18 Vented Peak	R16 Hip/Ridge	R17 Vented Ridge	R18 Narrow Ridge	
Varies

Varies

1/2"
Pitch Required	
Varies
Varies
1-1/8"  2"

1/2"	Pitch Required	
5-1/2"

Pitch Required	
6-3/4"
1-1/8"	2"

Pitch Required	
4-7/16"
7/8"

Pitch Required	

SS1 Starter Strip	SW16 Sidewall	SW17 Sidewall	SW18 Sidewall	TR16 Transition (High-Low)	TR17 Transition (Low-High)	

1"

2-1/2"	

4"
2-1/4"
1-1/8"	3/4"	

4"
2-1/4"

2-1/8"  3/4"	
4"	

2-1/4"	
5"
Varies

Pitch Required	

Varies	5"

Pitch Required	
			
1"	2-1/2"			

V16 Valley	Z17 Solid Zee Closure	Z18 Perforated Zee	B1 Base Trim	

1"
12"

Pitch Required	
2-13/16"
1-3/16"	Colors may vary 1"
Pitch Required	1-3/16"	Varies

1"
Pitch Required	

2-1/8"

1"	1/2"	

C13 C-Metal	G19 Gable	IC2 Inside Corner	OC2 Outside Corner	

3-1/2"

1"
1"	3-1/2" 1/2"
4-3/4"

3/4"	

3-1/2"	

3-1/2"	

SW8 Sidewall

E6 Eave
5-3/4"

EW6 Endwall

R8 Ridge

5-1/4"

4-1/2"

10"

5"

4"

6"

Pitch Required

3/4"

Pitch Required

Pitch Required

V6 W-Valley	B6 Drip Edge	C6 C-Metal	G8 Gable	

3/4"
20-3/4"

Pitch Required	

4-1/8"
1-5/8"
3/4"	
3-7/8"

1-3/8"

1-1/4"	4-7/8"	7/8"
1-3/4"
1/2"
5-1/4"

3/4"	

G9 Sculptured Gable	IC7 Inside Corner	OC7 Outside Corner	SW7 Sidewall	
6"
1"  2-1/8"	3-1/2"
5/8"
1-1/2"  3-1/2"
2-1/8"	

4-1/4"
1-3/4"
3/4"	

4-3/16"

1-15/16"
5/8"	

5-5/8"
5"
2-1/8"  1"	

Strata Rib 	Nor-Clad 	Delta Rib III 	Delta Rib 	21⁄2 Corrugated
B1 Base Trim	C1 7/8” C-Metal	E1 Eave	E2 Eave	E3 Eave	E4 Eave	

2-1/8"

1"  1/2"	2"

7/8"

1"	1-1/2"

3"

1/2"
Pitch Required	2"

4-3/8"

Pitch Required	1/2"	1-3/8"

1-3/8"
1/2"
Pitch Required	2"

2"

Pitch Required	1/2"	

E5 Eave	ER1 Residential 3” Eave	ER2 Residential 4” Eave	EW1 Endwall	EW2 Residential Endwall	EW17 Vented Endwall	
3"

3"
1/2"
Pitch Required	2"

3-3/8"

1/2"
Pitch Required	3"

4-3/8"

1/2"
Pitch Required	
4"
1-1/8"
1/2"	2"
1/2"  3/4"
Pitch Required	

4"

5"
Pitch Required	
4"
6-3/4"

1-1/8" 1-7/8"	

G1 Gable	G3 Gable	G4 Residential Gable	G18 Chalet Gable	IC1 Inside Corner	
4" 1-1/8" 5/8"
5"

5/8"
3/8"	4"
1-1/4"  1/2"
2-3/4"

1/2"	2"	5/8"
1-1/8" 3/8"
4"

1/2"	3/4"
1-5/8"  6"
3-7/8"
5/8"	

4"
1-1/8"
5/8"	

IC2 Inside Corner	OC1 Outside Corner	OC2 Outside Corner	PB3 Pitch Break (High-Low)	PB4 Pitch Break (Low-High)	

3-1/2"	

4"

1-1/8"
5/8"	

3-1/2"	

5"

6"

Pitch Required	
6"
5"

Pitch Required	

PF2 Peak Flashing	PF3 Vented Peak	R1 Ridge	R2 Vented Ridge	
Varies

Varies	3/8"

1/2"
Pitch Required	
Varies
Varies
1-1/8" 1-7/8"
1/2"
Pitch Required	
2"	2-1/8"
1/2"	1-7/8"
1/2"
13/16"	

6-3/4"
1-1/8"	1-7/8"	

R3 Standard Ridge	R4 Residential Ridge	SW1 Sidewall	SW2 Residential Sidewall	

7"	

3-3/4"
3-1/2"
1/2"	

4"
1/2"	1/2"
1-1/8"	2"	3/4"	

4"
3"
1-1/8" 5/8"	

TC1 Single Track Cover	TC2 Single Track Cover	TC3 Double Track Cover	V1 W-Valley	V2 Residential Valley	
1-1/2"  3-13/16"
1-7/16"

3-13/16"	1-1/2"
2-1/4"	1-7/16"

3-13/16"	1-1/2"

7-3/16"
2-1/2"
2-3/8"	
1"
13"

Pitch Required	

1"	19-7/16"

Pitch Required	

®

Trims and Flashings Guide

Customer Service Centers
Salem, OR: 503-390-7174 or 800-272-7023 I Spokane, WA: 509-536-4097 or 800-776-8771
PS328 0225 web

www.ascbp.com