®

Trims and Flashings Guide

5-1/2" | 2"
6" |

Refer to the color key for the most common trims and flashings available by product.
Design Span hp 	Skyline Roofing 

L41 Closure | OL41 Offset Cleat | R16 Hip/Ridge | R18 Narrow Ridge

1-3/4"
2-1/4"

1-1/2"

_5/16"	13/16"

5-1/2"

Pitch Required

4-7/16"

7/8"

Pitch Required

AL41 Angle Cleat | ZL41 “Z” Clip | R17 Vented Ridge | Z16 Perforated Zee

2-3/8"

5/8"

2 1/8"
1-3/4"

^2” ^Length	2 1/8"

6-3/4"
1-1/8"  ^2"

Pitch Required

Varies

^1-3/16"	Colors may vary 1"
Pitch Required

Z41 “Z” Closure | R41 Ridge | Z17 Solid Zee Closure | G16 Narrow Gable

2-1/8"
1-3/4"

2-1/8"

8-1/2"

Pitch Required

2-13/16"
1-3/16"
Colors may vary
1"

Pitch Required

1/2"
1"	1"

3"
1/2"

R42 Vented Ridge | V41 Valley | G17 Standard Gable | G18 Chalet Gable

9"
1-1/2"  ^3"

Pitch Required

1/2"
^1"	19-1/2"

Pitch Required

2-1/4"
1-1/8"	^3/4"
_4"	3/8"
1/2"

^3/4"	1-5/8"
3-7/8"	^6"

5/8"

G41 Gable | SF41 Support Flashing | V16 Valley | E16 Narrow Eave

1-1/2"
1-1/4"
1/2"
5-7/8"

3/4"

1"

1-3/4"

5-1/4"

1"
12"

Pitch Required

2"

1-1/8"

Pitch Required	^1/2"

CF41 Counter Flashing | B41 Drip Flashing | E17 Wide Eave | E18 Snow Eave

3-1/2"

1"
1"

2"

4"

3"
Pitch Required	^5/8"

5-1/8"

1-1/4"
1-3/4"
Pitch Required	^1/2"

TR41 Transition (High-Low) | TR43 Transition (Low-High) | E19 Notched Eave | TR16 Transition (High-Low)

^7"	16-1/2"

Pitch Required

16-1/2"
7"

Pitch Required

3-1/4"

No customs		_1-1/4" available	_Varies

5/8"
Pitch Required

5"
Varies

Pitch Required

Refer to the color key for the most common trims and flashings available by product.
Skyline Roofing 	Nu-Wave Corrugated  	PBR Pannel

TR17 Transition (Low-High) | SW16 Sidewall | SW17 Sidewall | SW18 Sidewall

Varies	_5"

Pitch Required

4"
2-1/4"
1-1/8"  ^3/4"

4"
2-1/4"
2-1/8"  ^3/4"

4"

2-1/4"

1" | 2-1/2"

EW16 Endwall | EW17 Vented Endwall | B16 Base Trim | PF16 Peak Flashing

4"

5-1/2"

Pitch Required

4"
6-3/4"
_1-1/8"	1-7/8"
Pitch Required

3"

1-1/8"
1/2"

Varies
Varies 1/2"
Pitch Required

C13 C-Metal | EW6 Universal Endwall | SW7 Sidewall | G8 Gable

3-1/2"

1"
1"

4-1/2"

6"
Pitch Required

5-5/8"

5"
2-1/8"  ^1"

4-7/8"	_7/8"
1-3/4"
5-1/4"	^1/2"

3/4"

G19 Gable | V6 W-Valley | OC7 Outside Corner | IC7 Inside Corner

3-1/2"  _1/2"
4-3/4"

3/4"

3/4"
20-3/4"
Not available for PBR Panel

Pitch Required

4-3/16"

1-15/16"
5/8"

4-1/4"

1-3/4"

3/4"

IC11 Universal Inside Corner | R8 Ridge | C6 C-Metal | G9 Sculptured Gable

6-3/4"

10"

Pitch Required

3-7/8"

1-3/8"

1-1/4"

6"
^1"	2-1/8"	3-1/2"
5/8"
1-1/2"  ^3-1/2"
2-1/8"

OC11 Universal Outside Corner | E6 Eave

6-3/4"

5-3/4"

4"
Pitch Required	^3/4"

BOTTOM CLOSURE

VALLEY FLASHING

GABLE TRIM

UNIVERSAL ENDWALL

UNIVERSAL HIP/RIDGE

EAVE FLASHING

Pitch Required = Trim manufactured based on roof pitch. Please ensure roof pitch provided at time of order entry.

SW8 Sidewall | B6 Drip Edge

5-1/4"

5"

4-1/8"

1-5/8"
3/4"

UNIVERSAL SIDEWALL

TOP CLOSURE

PIPE FLASHING

®

Trims and Flashings Guide

www.ascbp.com

Refer to the color key for the most common trims and flashings available by product. Strata Rib 	Nor-Clad 	Delta Rib III 	Delta Rib 	2^1⁄2 Corrugated 
R1 Universal Ridge | R3 Standard Ridge | R4 Residential Ridge | R2 Vented Ridge

^2"	2-1/8"
_1/2"	1-7/8"
1/2"
13/16"

7"

Pitch Required

3-3/4"
1/2"	3-1/2"

Pitch Required

6-3/4"
_1-1/8"	1-7/8"

Pitch Required

C1 7/8” C-Metal | V1 W-Valley | V2 Residential Valley | B1 Base Trim

2"

7/8"

1"

1"
13"

Pitch Required

^1"	19-7/16"

Pitch Required

2-1/8"

^1"	1/2'

E1 Eave | E2 Eave | E3 Eave | E4 Eave | E5 Eave

1-1/2"

3"

1/2"
Pitch Required

2"

4-3/8"

Pitch Required	^1/2"

1-3/8"

1-3/8"

1/2"
Pitch Required

2"

2"

1/2"
Pitch Required

3"

3"
1/2"
Pitch Required

ER1 Residential 3” Eave | ER2 Residential 4” Eave | G1 Gable | G3 Gable | G4 Residential Gable

2"

3-3/8"

Pitch Required	^1/2"

3"

4-3/8"

Pitch Required	^1/2"

^4"  1-1/8" ^5/8"
5"

5/8"
3/8"

4"
1-1/4"	^1/2"
2-3/4"

1/2"

^2"	5/8"
1-1/8" _3/8"
4"

1/2"

PF2 Peak Flashing | OC1 4” x 4” Outside Corner | OC2 Universal Outside Corner | IC1 4” x 4” Inside Corner

Varies

Varies	_3/8"

Pitch Required  ^1/2"

4"

1-1/8"

5/8"

3-1/2"

4"
1-1/8"
5/8"

IC2 Universal Inside Corner | SW1 Universal Sidewall | SW2 Residential Sidewall | EW1 Universal Endwall

3-1/2"

4"
1/2"	_1/2"
^1-1/8"	2"	3/4"

4"
3"
1-1/8"	^5/8"

4"
1-1/8"
1/2"	_2"
1/2"	3/4"
Pitch Required

EW2 Residential Endwall | PB3 Pitch Break (High-Low) | PB4 Pitch Break (Low-High) | SB1 Snow Break

4"

5"
Pitch Required

5"

6"

Pitch Required

6"
5"

Pitch Required

3-1/2"
^2"	1-1/2"

Works with most panels

Customer Service Centers
Salem, OR: 503-390-7174 or 800-272-7023 I Spokane, WA: 509-536-4097 or 800-776-8771
PS328 0224 web