PBR Panel is ideal for pre-engineered metal, post-frame, and agricultural buildings. PBR Panel offers a unique yet flexible design when combined with other building materials is perfect for use in buildings for livestock and animal confinement.

FEATURES AND BENEFITS:
36" coverage roof and wall panel.
Roof Installation: Minimum recommended 1:12.
Wall Installation: Horizontal or Vertical.
26ga in Dura Tech™ nt, 24ga in Dura Tech™ 5000/mx.
Custom manufactured panel lengths: 5'-0" to 40'-0".
Matching polycarbonate panels available.
See website for testing and certifications.

DURA TECH™ MX (PVDF) Subject to upcharge.

DURA TECH™ NT (SMP) 26 Gauge

  
Metallic Silver	ZACtique® II  Metallic Champagne
SRI 65 | LRV 50	SRI 39 | LRV 22	SRI 54 | LRV 33
Slate Gray	Matte Black	Tahoe Blue	Regal Blue	Sage Green
SRI 33 | LRV 12	SRI 29 | LRV 5	SRI 33 | LRV 14	SRI 29 | LRV 10	SRI 41 | LRV 21

11⁄

36" net coverage

Leaf Green

12"

					
ZINCALUME® Plus SRI 64 | LRV 67	Winter White
SRI 88 | LRV 74	Surf White
SRI 74 | LRV 59	Light Stone
SRI 70 | LRV 53	Desert Beige
SRI 58 | LRV 39	
					
Chestnut Brown	Rustic Red
SRI 36 | LRV 12	SRI 43 | LRV 13	Old Town Gray
SRI 43 | LRV 27	Tahoe Blue
SRI 33 | LRV 14	Weathered Copper
SRI 32 | LRV 11

Weathered Copper
SRI 34 | LRV 11

Zinc Gray
SRI 39 | LRV 20	

Denali Green
SRI 29 | LRV 11
DURA TECH™ 5000 (PVDF) 24 Gauge				
					
ZINCALUME® Plus SRI 64 | LRV 67	Regal White
SRI 88 | LRV 75	Parchment
SRI 58 | LRV 40	Sierra Tan
SRI 55 | LRV 34		
					
Dark Bronze
SRI 32 | LRV 8	Terra-Cotta
SRI 41 | LRV 15	Colonial Red
SRI 35 | LRV 9	Old Town Gray
SRI 43 | LRV 27		

SRI 30 | LRV 11

Forest Green
SRI 29 | LRV 9

Customer Service Centers
Salem, OR: 503-390-7174 or 800-272-7023 I Spokane, WA: 509-536-4097 or 800-776-8771

www.ascbp.com

PBR Panel

®

4"	Representation of colors may vary due to printing limitations.
Sample color chips are available upon request.