®
Polycarbonate Panels

POLYCARBONATE SKYLIGHT & SIDELIGHT PANELS
SUNSKY Polycarbonate Panels offer multiple advantages over traditional

fiberglass corrugated panels. Designed specifically to withstand punishing climates and harsh exterior conditions, they are ideal for agricultural, patio cover, and industrial workshop applications.
Features and Benefits:
Polycarbonate panels are virtually unbreakable, offering up to 20 times greater impact resistance compared to a fiberglass panel.
Panels retain optical clarity far better than any other glazing material for increased light transmission, while offering 100% UV protection. UV protection is only on the
standard (non-reversed) side of the panel.
Panel profiles can handle extreme climates (-40°F to 270°F).
Easily and safely installed.
Panel provides highest resistance to wind uplift (UL 580 Class 90) and hail protection.

Panel	Length	Thickness	Color	
PBR Panel	12'	8mm	White	
Nu-Wave® Corrugated	12'	8mm	White	
2.5" Corrugated	8', 10', 12'	8mm	Clear & White	
Nor-Clad®	2', 8', 10', 12'	8mm	Clear & White	
Strata Rib®	2', 8', 10', 12'	8mm	Clear & White	
Delta Rib™	2', 8', 10', 12'	8mm	Clear & White	
Delta Rib III™	2', 8', 10', 12'	8mm	Clear & White	

All panels come with 10-Year warranty.

SUNSKY Polycarbonate panels match up to ASC Building Products most popular metal panel profiles.

SUNSKY is a registered trademark of PALRAM Industries LTD.

Illustration not representative of actual profile

Contact your ASC Building Products Representative for more information.

Customer Service Centers
Salem, OR: 503-390-7174 or 800-272-7023 I Spokane, WA: 509-536-4097 or 800-776-8771
©2016-2023 ASC Profiles LLC.  All rights reserved. 0224  web  (PS324)

www.ascbp.com