SKYLINE ROOFING® hp	®

Skyline Roofing hp

STANDING BY OUR PRODUCTS AND WARRANTIES FOR OVER 50 YEARS

Skyline Roofing hp

Customer Service Centers
Salem, OR: 503-390-7174 or 800-272-7023 I Spokane, WA: 509-536-4097 or 800-776-8771

www.ascbp.com

Skyline Roofing hp is a 24 gauge high-
performance panel available in durable premium colors. This concealed fastener, standing
seam panel is ideal for residential and light- commercial roof applications.
FEATURES AND BENEFITS
Available in our Dura Tech™ 5000 and Dura Tech™ mx colors, which are energy efficient, cool colors, formulated to help reduce the demand for energy.
Limited Lifetime Warranty for residential applications.

ASTM E1592 tested for wind uplift performance.
Skyline Roofing hp panel assemblies are Class
A Fire Rated when installed on non-combustible

deck or framing per IBC, IRC, or UL790 when installed in accordance to UL listings.
Panel evaluated by accredited third party.

All structural performance data is contained within an IBC/IRC 2015 code compliance report.

 1"

 1"

16" Net Coverage

Skyline Roofing hp (Striated Option)
(Additional Lead Times May Apply)

16" Net Coverage

®
5000

®
5000

Standard Offer	Special Order (Minimum order required)

Cool Forest Green SRI: 29 • LRV: 9

Cool Dark Bronze SRI: 32 • LRV: 8

Cool Matte Black SRI: 29 • LRV: 5

Cool Walnut SRI: 38 • LRV: 18

Cool Pebble SRI: 48 • LRV: 27

Cool Parchment SRI: 58 • LRV: 40

Cool Sierra Tan SRI: 55 • LRV: 34

  	   

Cool Slate Gray SRI: 33 • LRV: 12

Cool Old Town Gray SRI: 43 • LRV: 27

Cool Zinc Gray SRI: 39 • LRV: 20

Cool Sage Green SRI: 41 • LRV: 21

Cool Leaf Green SRI: 30 • LRV: 11

Cool Midnight Bronze SRI: 27 • LRV: 7

Cool Tahoe Blue SRI: 33 • LRV: 14

Cool Weathered Copper SRI: 34 • LRV: 11

Special Order (Minimum order required)

Cool Colonial Red SRI: 35 • LRV: 9

ZINCALUME® Plus SRI: 64 • LRV: 67

Cool Terra-Cotta SRI: 41 • LRV: 15

Cool Regal Blue SRI: 29 • LRV: 10

Cool Regal White SRI: 88 • LRV: 75

Cool Metallic Copper*
SRI: 53 • LRV: 29

Cool Silversmith* SRI: 58 • LRV: 54

Cool Metallic Champagne* SRI: 54 • LRV: 33

Cool ZACtique® II* SRI: 39 • LRV: 22

Cool Metallic Silver*

SRI: 65 • LRV: 50

REPRESENTATION OF COLORS MAY VARY DUE TO PRINTING LIMITATIONS.
Sample color chips are available upon request. Consult your ASC Building Products representative for more information.

Oil Canning
All flat metal surfaces can display waviness commonly referred to as

METAL ROOFING

EXCELLENCE IN

ASC Building Products is Proudly Distributed by:

All information stated in the product sheet is correct at time of printing and subject to change without

www.ascbp.com

SKYLINE ROOFING® hp

®

* Metallic colors are subject to price upcharge. These colors are batch sensitive (may have color variation) and are directional in nature. Different batches are not to be mixed on projects. We recommend you request a sample of current stocked material to review actual color before ordering to ensure color accuracy.

“oil canning.” “Oil canning” is an inherent characteristic of steel products, not a defect, and therefore is not a cause for panel rejection.